Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# vlan bulk-config modify

#### Syntax

To modify VLAN ranges containing single-tagged VLAN IDs:

vlan bulk-config bulkConfigName modify vlan-range vlanIdStart vlanIdEnd

To modify VLAN ranges containing double-tagged S-VLAN IDs or based on agent-circuit-identifier:

vlan bulk-config bulkConfigName modify svlan-range s-vlanIdStart s-vlanIdEnd
{ vlanIdStart vlanIdEnd | any | agent-circuit-identifier }

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Modifies the VLAN subrange values for the specified bulk configuration VLAN range. If the new subrange encompasses previously configured subranges within that range, those subranges are merged into the new one, freeing subrange resources. There is no no version.

#### Options

- bulkConfigName—Name of the VLAN range; string of up to 80 characters
- vlanIdStart—Starting VLAN ID of the VLAN subrange you are configuring
- vlanIdEnd—Ending VLAN ID of the VLAN subrange you are configuring
- s-vlanIdStart—Starting S-VLAN ID of the S-VLAN subrange you are configuring
- s-vlanIdEnd—Ending S-VLAN ID of the S-VLAN subrange you are configuring
- any—Specifies the VLAN ID as a wildcard
- agent-circuit-identifier—Specifies a VLAN range that is based on agent-circuit-identifier information

#### Mode

Interface Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out