# radius acct-session-id-format

#### Syntax

radius acct-session-id-format { decimal | description }

no radius acct-session-id-format

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the RADIUS client’s use of a specific format for RADIUS attribute 44, Acct-Session-Id. The no version negates the Acct-Session-Id format.

| Note: For subscribers connected over the link aggregation group (LAG) interface in DHCP standalone authenticate mode, the LAG interface ID is used as the interface identifier.

#### Options

- decimal—Configures the RADIUS client to use a decimal format
- description—Configures the RADIUS client to use the generic format:
  erx interfaceType interfaceSpecifier:hexNumber
  - interfaceType—Interface type; see Interface Types and Specifiers
  - interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
  - hexNumber—Hexadecimal number identifying the session

#### Mode

Global Configuration