# Configuring a Parameter Definition to Adjust Cell Shaping Rates for ADSL Traffic

You can adjust shaping rates to account for different layer 2 encapsulations as well as the ATM cell pad, header, and trailer on interfaces with cell shaping mode using the qos-byte-adjustment application.

| Note: When you apply a parameter with the qos-byte-adjustment application to an interface with frame shaping mode, you adjust shaping rates to account for different layer 2 encapsulations only.

To associate a parameter instance with the byte adjustment application:

1. Configure the traffic classes.
   host1(config)#traffic-class voice host1(config-traffic-class)#exit host1(config)#traffic-class best-effort host1(config-traffic-class)#exit
2. Create a parameter definition.
   1. Configure the QoS parameter name and the application.
      host1(config)#qos-parameter-define byteadjust1 application qos-byte-adjustment
   2. Configure a controlled-interface type.
      host1(config-qos-parameter-define)#controlled-interface-type vlan host1(config-qos-parameter-define)#controlled-interface-type ip
   3. Configure an instance-interface type.
      host1(config-qos-parameter-define)#instance-interface-type vlan
3. Do one of the following:
   - Configure the shaping mode by issuing the qos-shaping-mode command.

     Frame shaping mode is the default for Ethernet interfaces on all E Series routers. You can only set the cell shaping mode for Gigabit Ethernet and 10-Gigabit Ethernet interfaces configured on the GE-2 line module, the GE-HDE line module, and the ES2 4G LM.

   - Configure the shaping mode by specifying the QoS cell mode application with a parameter definition.
     host1(config)#qos-parameter-define cell-mode application qos-cell-mode
4. Attach the parameter definition to a logical Ethernet interface.

   In this example, parameter instances are created for both the byte adjustment and QoS cell mode applications.

   host1(config)#interface gigabitEthernet 7/0 host1(config-if)#encapsulation vlan host1(config-if)#exit host1(config)#interface gigabitEthernet 7/0.1 host1(config-if)#vlan id 1 host1(config-if)#qos-parameter byteadjustment -16 host1(config-if)#qos-parameter cell-mode 1 host1(config-if)#ip address 1.1.1.1 255.255.255.0

#### Related Documentation

- Byte Adjustment for ADSL and VDSL Traffic Overview
- Guidelines for Configuring Byte Adjustment of Cell and Frame Shaping Rates Using QoS Parameters
- Example: QoS Parameter Configuration for QoS Cell Mode and Byte Adjustment for Cell Shaping
- For information about managing packet fragmentation for traffic with frame shaping mode, see Configuring a Parameter Definition to Adjust Frame Shaping Rates for VDSL Traffic
- For more information about configuring shaping modes for Ethernet, see QoS Shaping Mode for Ethernet Interfaces Overview and Cell Shaping Mode Using QoS Parameters Overview
- controlled-interface-type
- encapsulation vlan
- instance-interface-type
- ip address
- node
- qos-parameter
- qos-parameter-define
- qos-profile
- queue
- traffic-class
- vlan id