Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ICR Terms

Table 1 defines terms used in this discussion of ICR.

Table 1: ICR Terminology

Term | Description
--- | ---
ICR cluster | Group of E Series routers participating in interchassis redundancy (ICR) deployment.
ICR interface | Physical interface, for example, gigabitEthernet 3/1/3, on an E Series router on which ICR is enabled. The ICR interface is always tied to a unique router.
ICR partition | A logical group of subscriber interfaces within a single ICR interface. For example, the ICR partition can be a group of S-VLANs configured on a single physical interface. You can create multiple partitions on each ICR interface and configure the number of partitions, as well as assign subscribers to the partition. An ICR partition can be configured as master or backup.
VRRP | Virtual Router Redundancy Protocol. Use VRRP to prevent loss of network connectivity by configuring backup routers. The backup routers maintain network connectivity when the master router fails. You can configure unique VRRP instances to manage each ICR partition.
VSA | Vendor-specific attributes. VSAs are defined by remote-access server vendors to customize how RADIUS works on their servers. VSAs can be used in combination with RADIUS-defined attributes.

#### Published: 2011-10-18

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out