Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ipv6 nd prefix-advertisement

#### Syntax

ipv6 nd prefix-advertisement ipv6Prefix/ipv6PrefixLength validLifetime preferredLifetime
[ onlink ] [ autoconfig ]

[ no ] ipv6 nd prefix-advertisement [ ipv6Prefix/ipv6PrefixLength ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
Profile Configuration mode added in JunosE Release 9.0.0.

#### Description

Specifies which IPv6 prefixes the router includes in IPv6 router advertisements. In Profile Configuration mode, you can configure a single prefix. The no version removes any prefixes from the IPv6 routing advertisements.

#### Options

- ipv6Prefix—IPv6 network number to include in router advertisements
- ipv6PrefixLength—Length of the IPv6 prefix; a decimal value that indicates how many of the higher-order contiguous bits of the IPv6 address comprise the prefix (the network portion of the IPv6 address). A slash (/) must precede this value.

  | Note: When used in an IPv6 profile, the ipv6PrefixLength must be set to a length of 64.

- validLifetime—Amount of time in seconds that the router can advertise the specified IPv6 prefix as valid; in the range 0–4294967295
- preferredLifetime—Amount of time in seconds that the router can advertise the specified IPv6 prefix as preferred; in the range 0–4294967295
- onlink—Indicates that the specified prefix is assigned to the link
- autoconfig—Indicates that local host links can use the specified prefix for IPv6 autoconfiguration

#### Mode

Interface Configuration, Profile Configuration

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out