# DSL Forum VSAs

Table 57 describes the DSL Forum VSAs supported by JunosE Software for RADIUS. JunosE Software uses the vendor ID assigned to the DSL Forum (3561, or DE9 in hexadecimal format) by the Internet Assigned Numbers Authority (IANA).

Table 57: JunosE Software DSL Forum (Vendor ID 3561) VSA Formats

Attribute Number | Attribute Name | Description | Length | Subtype Length | Value
--- | --- | --- | --- | --- | ---
[26-1] | Agent-Circuit-Id | Identifier for the subscriber agent circuit ID that corresponds to the DSLAM interface from which subscriber requests are initiated | len | sublen | string: agent-circuit-id
[26-2] | Agent-Remote-Id | Unique identifier for the subscriber associated with the DSLAM interface from which requests are initiated | len | sublen | string: agent-remote-id
[26-129] | Actual-Data-Rate- Upstream | Actual upstream data rate of the subscriber’s synchronized DSL link | 12 | 6 | integer: 4-octet
[26-130] | Actual-Data-Rate- Downstream | Actual downstream data rate of the subscriber’s synchronized DSL link | 12 | 6 | integer: 4-octet
[26-131] | Minimum-Data-Rate- Upstream | Minimum upstream data rate configured for the subscriber | 12 | 6 | integer: 4-octet
[26-132] | Minimum-Data-Rate- Downstream | Minimum downstream data rate configured for the subscriber | 12 | 6 | integer: 4-octet
[26-133] | Attainable-Data-Rate- Upstream | Upstream data rate that the subscriber can attain | 12 | 6 | integer: 4-octet
[26-134] | Attainable-Data-Rate- Downstream | Downstream data rate that the subscriber can attain | 12 | 6 | integer: 4-octet
[26-135] | Maximum-Data-Rate- Upstream | Maximum upstream data rate configured for the subscriber | 12 | 6 | integer: 4-octet
[26-136] | Maximum-Data-Rate- Downstream | Maximum downstream data rate configured for the subscriber | 12 | 6 | integer: 4-octet
[26-137] | Minimum-Data-Rate- Upstream-Low-Power | Minimum upstream data rate in low power state configured for the subscriber | 12 | 6 | integer: 4-octet
[26-138] | Minimum-Data-Rate- Downstream-Low-Power | Minimum downstream data rate in low power state configured for the subscriber | 12 | 6 | integer: 4-octet
[26-139] | Maximum-Interleaving- Delay-Upstream | Maximum one-way upstream interleaving delay configured for the subscriber | 12 | 6 | integer: 4-octet
[26-140] | Actual-Interleaving- Delay-Upstream | Subscriber’s actual one-way upstream interleaving delay | 12 | 6 | integer: 4-octet
[26-141] | Maximum-Interleaving- Delay-Downstream | Maximum one-way downstream interleaving delay configured for the subscriber | 12 | 6 | integer: 4-octet
[26-142] | Actual-Interleaving- Delay-Downstream | Subscriber’s actual one-way downstream interleaving delay | 12 | 6 | integer: 4-octet
[26-144] | Access-Loop- Encapsulation | Encapsulation used by the subscriber associated with the DSLAM interface from which requests are initiated | 11 | 5 | string: 3-byte
[26-254] | IWF-Session | Indication that the interworking function (IWF) has been performed for the subscriber’s session to enable the transport of PPP over ATM traffic on a PPPoE interface | 8 | 2 | No data field required