Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- ip policy-list

# Creating Policy Lists for IP

The following example creates an IP policy list named routeForABCCorp. For information about creating the CLACLs and rate-limit profile used in this example, see the previous sections.

1. Create the policy list routeForABCCorp.
   host1(config)#ip policy-list routeForABCCorp host1(config-policy-list)#
2. Create the classification group for the CLACL named ipCLACL10 and assign the precedence to the classification group.
   host1(config-policy-list)#classifier-group ipCLACL10 precedence 75 host1(config-policy-list-classifier-group)#
3. Add a rule that specifies a group of forwarding solutions based on classifier list ipCLACL10.
   host1(config-policy-list-classifier-group)#forward next-hop 192.0.2.12 order 10 host1(config-policy-list-classifier-group)#forward next-hop 192.0.100.109
   order 20 host1(config-policy-list-classifier-group)#forward next-hop 192.120.17.5 order 30 host1(config-policy-list-classifier-group)#forward interface ip 3/1 order 40
4. Add a rule that sets a ToS byte value of 125 for packets based on classifier list ipCLACL10.
   host1(config-policy-list-classifier-group)#mark tos 125
5. Add a rule that uses rate-limit profile ipRLP25.
   host1(config-policy-list-classifier-group)#rate-limit-profile ipRLP25
6. Exit Classifier Group Configuration mode for ipCLACL10, then create a new classification group for classifier list ipCLACL20. Add a rule that filters packets based on classifier list ipCLACL20.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#classifier-group ipCLACL20 precedence 125 host1(config-policy-list-classifier-group)#filter
7. Exit Policy List Configuration mode to save the configuration.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#exit host1(config)#
8. Display the policy list.

       host1#show policy-list routeForABCCorp

                                         Policy Table
                                         ------ -----
       IP Policy routeForABCCorp
          Administrative state: enable
          Reference count:      0
          Classifier control list: ipCLACL10, precedence 75
             forward
                Virtual-router: default
                List:
                  next-hop 192.0.2.12, order 10, rule 2 (active)
                  next-hop 192.0.100.109, order 20, rule 3 (reachable)
                  next-hop 192.120.17.5, order 30, rule 4 (reachable)
                  interface ip3/1, order 40, rule 5
             mark tos 125
             rate-limit-profile ipRLP25
          Classifier control list: ipCLACL20, precedence 125
             filter

## Related Documentation

- ip policy-list

#### Published: 2011-09-30

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out