Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring Rate Shaping for a Scheduler Node or Queue
- Configuring Port Shaping
- Configuring a Basic Parameter Definition for QoS Administrators

# shaping-rate

#### Syntax

shaping-rate shapingRate [ operator operandValue ]* [ bps | kbps ]
[ burst burstSize [ milliseconds | bytes ] ]

shaping-rate operandValue [ operator operandValue ]* [ bps | kbps ]

no shaping-rate

#### Release Information

Command introduced before JunosE Release 7.1.0.
milliseconds and bytes keywords added in JunosE Release 7.1.0.
bps and kbps keywords added in JunosE Release 8.0.0.

#### Description

Sets the shaping rate and burst size. The no version deletes the shaping rate.

#### Options

- shapingRate—Constant shaping rate in bits per second or kilobits per second; in the range 1–1000000000 bps/kbps. You can set the shaping rate to vary from 1 bps to 1000 gbps (which is denoted by entering 1000000000 kbps in the CLI for this command).
- operator—Mathematical function
- operandValue—Input for the operator; can be a QoS parameter definition name or an integer
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- bps—Specifies shaping rate in bits per second
- kbps—Specifies shaping rate in kilobits per second

  | Note: The lower and higher limits for the shaping rate range apply to both the bps and kbps keywords available with this command. For example, if you want to set the shaping rate to 1 mbps, you can either enter 1000 as the value for the shapingRate argument and suffix it with the kbps keyword, or enter 1000000 as the value for the shapingRate argument and suffix it with the bps keyword. Both the methods of configurations result in the same shaping rate value to be set.

- burstSize—Number, in the range 0–522240 (0–510 KB); 0 enables the router to select an applicable default value
- milliseconds—Specifies burst size in milliseconds
- bytes—Specifies burst size in bytes

#### Mode

Scheduler Profile Configuration

## Related Documentation

- Configuring Rate Shaping for a Scheduler Node or Queue
- Configuring Port Shaping
- Configuring a Basic Parameter Definition for QoS Administrators

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out