Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- show frame-relay subinterface

# Monitoring the Policy Configuration of Frame Relay Subinterfaces

#### Purpose

Display information about a subinterface’s Frame Relay policy lists.

#### Action

To display information about Frame Relay policy lists:

    host1#show frame-relay subinterface
    Frame relay sub-interface SERIAL5/0:1/1.1, status is up
    Number of sub-interface down transitions is 0
    Time since last status change 03:04:59
    No baseline has been set
      In bytes: 660                    Out bytes: 660
      In frames: 5                     Out frames: 5
      In errors: 0                     Out errors: 0
      In discards: 0                   Out discards: 0
      In unknown protos: 0
    Frame relay policy output frOutputPolicy
      classifier-group frGroupA entry 1
         5 packets, 640 bytes
         mark-de 1
    Frame relay sub-interface SERIAL5/1:1/1.1, status is up
    Number of sub-interface down transitions is 0
    Time since last status change 03:05:09
    No baseline has been set
      In bytes: 660                    Out bytes: 660
      In frames: 5                     Out frames: 5
      In errors: 0                     Out errors: 0
      In discards: 0                   Out discards: 0
      In unknown protos: 0
    Frame relay policy input frInputPolicy
      classifier-group frMatchDeSet entry 1
          5 packets, 660 bytes
          color red

#### Meaning

Table 1 lists the show frame-relay subinterface command output fields.

Table 1: show frame-relay subinterface Output Fields

Field Name | Field Description
--- | ---
Frame Relay policy | Type and name of the VLAN policy
mark-de | DE bit value
color | Color applied to packet flow for queuing: green, yellow, or red
classifier-group | Name of the classifier control list used by the policy
filter | Filter policy action
forward | Forward policy action
traffic class | Traffic class in the policy list
user-packet-class | User packet class in the policy list

## Related Documentation

- show frame-relay subinterface

#### Published: 2011-09-30

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out