Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# resource if-type

#### Syntax

[ no ] resource if-type { atm-active-sub-if | atm-sub-if | atm-vc | ip | ppp-link }
{ slot slot | system }
threshold { falling fallingValue | hold-down-time holdDownTime | rising
risingValue }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies threshold values for specific interface types on a slot or systemwide basis. The no version sets the threshold parameter to its default value (for rising, 90% of the maximum value of the resource; for falling, 1% of the maximum value of the resource; for hold-down time, 300 seconds).

| Caution: Do not specify a falling value larger than the specified rising value; do not specify a rising value smaller than the specified falling value.

#### Options

- atm-active-sub-if—Configures active ATM subinterfaces
- atm-sub-if—Configures both active and inactive ATM subinterfaces
- atm-vc—Configures ATM virtual circuits
- ip—Configures IP interfaces
- ppp-link—Configures PPP link interfaces
- slot—Number of the chassis slot in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), 0–13 (ERX14xx models), 0–5 (E120 router), and 0-16 (E320 router)
- For ERX7xx models, a number in the range 0–6; for ERX14xx models, a number in the range 0–13; for the ERX310 router, a number in the range 1–2; for the E120 router, a number in the range 0–5; for the E320 router, a number in the range 0–16
- fallingValue—Falling threshold for the resource, in the range 0–4294967295
- holdDownTime—Hold-down time for the resource, in the range 0–4294967295 seconds
- risingValue—Rising threshold for the resource, in the range 0–4294967295

#### Mode

Global Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out