Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Subscriber AAA Access Messages Overview
- Subscriber AAA Accounting Messages Overview
- Juniper Networks VSAs Supported for Subscriber AAA Access Messages
- Juniper Networks VSAs Supported for Subscriber AAA Accounting Messages
- CLI Commands Used to Include or Exclude Attributes in RADIUS Messages
- Juniper Networks VSAs
- Monitoring Included RADIUS Attributes
- radius include

# CLI Commands Used to Include ANCP-Related Juniper Networks VSAs in Access and Accounting Messages

You use the radius include command to specify information about ANCP, also known as L2C, that you want to include in the RADIUS Access-Request, Acct-Start, and Acct-Stop messages. Also, if you specify Acct-Stop messages, the router includes ANCP information in Interim-Acct messages that the router sends to RADIUS. By default, the router does not include the ANCP-related information provided by the Juniper Networks VSAs in RADIUS messages.

These Juniper Networks ANCP-related VSAs are based on definitions in GSMP extensions for layer2 control (L2C) Topology Discovery and Line Configuration—draft-wadhwa-gsmp-l2control-configuration-00.txt (July 2006 expiration).

| You must enable ANCP discovery with the discovery-mode command prior to configuring the radius include command with the ANCP-related VSAs. Configuring discovery mode enables the RADIUS authentication server to retrieve ANCP information. JunosE Software continues to support DSL Forum VSAs (vendor ID 3561) that you can use to include DSL-related information in RADIUS messages. See DSL Forum VSAs.

Table 1 lists the ANCP (L2C)-related keywords that you can use in the radius include command and the associated Juniper Networks VSAs. The table also indicates the mappings between ANCP parameters and the VSAs.

Table 1: ANCP (L2C)-Related Keywords for radius include Command

Command Keyword | Juniper Networks VSA Number | Juniper Networks VSA Name | ANCP Type | ANCP Subtype
--- | --- | --- | --- | ---
l2cd-acc-loop-cir-id | [26-110] | Acc-Loop-Cir-Id | 1 | –
l2cd-acc-aggr-cir-id-bin | [26-111] | Acc-Aggr-Cir-Id-Bin | 2 | –
l2cd-acc-aggr-cir-id-asc | [26-112] | Acc-Aggr-Cir-Id-Asc | 3 | –
l2cd-act-data-rate-up | [26-113] | Act-Data-Rate-Up | 4 | 129
l2cd-act-data-rate-dn | [26-114] | Act-Data-Rate-Dn | 4 | 130
l2cd-min-data-rate-up | [26-115] | Min-Data-Rate-Up | 4 | 131
l2cd-min-data-rate-dn | [26-116] | Min-Data-Rate-Dn | 4 | 132
l2cd-att-data-rate-up | [26-117] | Att-Data-Rate-Up | 4 | 133
l2cd-att-data-rate-dn | [26-118] | Att-Data-Rate-Dn | 4 | 134
l2cd-max-data-rate-up | [26-119] | Max-Data-Rate-Up | 4 | 135
l2cd-max-data-rate-dn | [26-120] | Max-Data-Rate-Dn | 4 | 136
l2cd-min-lp-data-rate-up | [26-121] | Min-LP-Data-Rate-Up | 4 | 137
l2cd-min-lp-data-rate-dn | [26-122] | Min-LP-Data-Rate-Dn | 4 | 138
l2cd-max-interlv-delay-up | [26-123] | Max-Interlv-Delay-Up | 4 | 139
l2cd-act-interlv-delay-up | [26-124] | Act-Interlv-Delay-Up | 4 | 140
l2cd-max-interlv-delay-dn | [26-125] | Max-Interlv-Delay-Dn | 4 | 141
l2cd-act-interlv-delay-dn | [26-126] | Act-Interlv-Delay-Dn | 4 | 142
l2cd-dsl-line-state | [26-127] | DSL-Line-State | 4 | 143
l2cd-dsl-type | [26-128] | DSL-Type | 4 | 144

## Related Documentation

- Subscriber AAA Access Messages Overview
- Subscriber AAA Accounting Messages Overview
- Juniper Networks VSAs Supported for Subscriber AAA Access Messages
- Juniper Networks VSAs Supported for Subscriber AAA Accounting Messages
- CLI Commands Used to Include or Exclude Attributes in RADIUS Messages
- Juniper Networks VSAs
- Monitoring Included RADIUS Attributes
- radius include

#### Published: 2011-10-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out