# Configuring the NAS-Port-Type Attribute Manually

You can manually configure the NAS-Port-Type RADIUS attribute (attribute 61) in AAA profiles for ATM and Ethernet interfaces. Doing so allows AAA profiles to determine the NAS port type for a given connection.

To set the NAS-Port-Type attribute for ATM or Ethernet interfaces:

1. Create an AAA profile.
   host1(config)#aaa profile nasPortType
2. (Optional) Set the NAS-Port-Type attribute for ATM interfaces.
   host1(config-aaa-profile)#nas-port-type atm wireless-80211
3. (Optional) Set the NAS-Port-Type attribute for Ethernet interfaces.
   host1(config-aaa-profile)#nas-port-type ethernet wireless-cable