# radius pppoe nas-port-format unique

#### Syntax

[ no ] radius pppoe nas-port-format unique

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Allows the E Series RADIUS client to use a unique value for the NAS-Port attribute for subscribers on PPPoE interfaces. The router derives the unique value from the subscriber’s profileHandle. The no version restores the default value, determined by the interface.

| Note: For subscribers connected over the link aggregation group (LAG) interface in DHCP standalone authenticate mode, RADIUS derives a unique value from the subscriber’s profileHandle and uses the value for the Nas-Port attribute. You cannot use this command to change the value of the Nas-Port attribute.

#### Mode

Global Configuration