Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring Interface Sets for QoS

# member-interface-type

#### Syntax

member-interface-type {vlan | atm-vc | ip}

no member-interface-type

#### Release Information

Command introduced in JunosE Release 9.2.0.

#### Description

Configures the member-interface type for a QoS interface set. The no version removes the member-interface type from the parameter definition.

#### Options

- vlan—Specifies the member-interface-type as VLAN
- atm–vc—Specifies the member-interface-type as VLAN
- ip—Specifies the member-interface-type as VLAN

#### Mode

QoS Interface Set Configuration

#### Related Topics

- Configuring Interface Sets for QoS

#### Published: 2010-07-19

Help
|
My Account
|
Log Out