Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring CLI-Based Mirroring

# ip mirror

#### Syntax

ip mirror mirrorInterfaceType mirrorInterfaceSpecifier
[ analyzerInterfaceType analyzerInterfaceSpecifier [ next-hop nextHop ] ]

no ip mirror mirrorInterfaceType mirrorInterfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the specified interface to mirror all IP ingress and egress traffic, and directs the mirrored traffic to an analyzer interface. The no version disables mirroring on the interface.

| Note: This command is deprecated and might be removed completely in a future release. The function provided by this command has been replaced by the updated packet mirroring feature and the ip policy command used with the secure-input and secure-output keywords.

#### Options

- mirrorInterfaceType—Interface type; see Interface Types and Specifiers
- mirrorInterfaceSpecifier—Particular interface that performs the interface mirroring function; see Interface Types and Specifiers
- analyzerInterfaceType—Interface type
- analyzerInterfaceSpecifier—Particular interface used as the analyzer interface; if omitted, the virtual router's default analyzer interface is used
- nextHop—Next-hop IP address to the remote analyzer host; required if the analyzer interface is a shared medium, such as Ethernet

#### Mode

Global Configuration

#### Related Topics

- Configuring CLI-Based Mirroring

#### Published: 2010-07-19

Help
|
My Account
|
Log Out