Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# set route-type

#### Syntax

set route-type { internal | internal-intra | internal-inter | external }

no set route-type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets routes of the specified type. The no version removes the set clause from a route map.

#### Options

- internal—Internal route (including OSPF intra-area and interarea)
- internal-intra—Intra-area route
- internal-inter—Interarea route
- external—External route (BGP and OSPF type 1/2)

#### Mode

Route Map Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out