Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show l2tp dial-out target

#### Syntax

show l2tp dial-out target [ targetIpAddress targetIpAddressMask | allVirtualRouters ]
[ detail ] [ state operState ] [ filter ]

To display summary information:

show l2tp dial-out target summary [ allVirtualRouters ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays configured dial-out targets within the current virtual router context.

#### Options

- targetIpAddress—Trigger IP address for the target that you want to display
- targetIpAddressMask—Mask for the trigger IP address
- allVirtualRouters—Displays dial-out information for all virtual routers
- detail—Displays configuration, state, and statistics
- operState—One of the following operational states:
  - down
  - inService
  - inhibited
- filter—See Filtering show Commands
- summary—Displays aggregate counts for targets in each of the possible operational and administrative states

#### Mode

Privileged Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out