# ospfPktsRcvd

#### Description

OSPF packet received

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

None

#### Warning Log

Packets discarded; validation errors

#### Notice Log

Number of LSAs packed in different packet types (LSA Ack, LSA update); packets received over Down interface

#### Info

None

#### Debug

Packets received description

#### Filter 1

interface-ip-address—See description of the ospfElectDr interface-ip-address filter for information about this filter

#### Filter 2

router—See description of the ospfElectDr router filter for information about this filter