# atm classifier-list

#### Syntax

atm classifier-list classifierName [ traffic-class trafficClassName ]
[ color { green | yellow | red } ] [ user-packet-class userPacketClassValue ]
[ clp clpValue ]

no atm classifier-list classifierName [ classifierNumber ]

#### Release Information

Command introduced in JunosE Release 7.1.0.

#### Description

Creates a classifier control list that can only be used in ATM policy lists. The no version removes the ATM classifier control list. ATM packets are classified on CLP. The CLP bit is not available on frame-based interfaces on E Series Broadband Services Router line modules.

#### Options

- classifierName—Name of the classifier control list entry
- trafficClassName—Name of the traffic class to match
- green—Matches packet color to green, indicating a low drop preference
- yellow—Matches packet color to yellow, indicating a medium drop preference
- red—Matches packet color to red, indicating a high drop preference
- userPacketClassValue—User packet value to match in the range 0–15
- clpValue—Value of the CLP, 0 or 1
- classifierNumber—Index of the classifier control list entry to be deleted

#### Mode

Global Configuration

#### Related Topics

- Creating or Modifying Classifier Control Lists for ATM Policy Lists