Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups
- Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups
- Creating Parameter Instances
- For more information about other fields displayed with this command, see the JunosE Physical Layer Configuration Guide
- show interfaces lag members

# Monitoring the QoS Configuration of IEEE 802.3ad Link Aggregation Group Bundles

#### Purpose

Display information about the QoS configuration for Ethernet member links in all IEEE 802.3ad link aggregation group (LAG) bundles configured on the router, or about the member links in a specified IEEE 802.3ad LAG bundle.

#### Action

To display the QoS configuration for a specific LAG bundle:

    host1#show interfaces lag lg0 members
    Lag lg0 is Up, Administrative status is Up
    MAC Address is 0090.1a40.01be
    MTU: Operational 1526
    Duplex Mode: Operational Full Duplex
    Speed: Operational 100 Mbps
    System Priority 32768 System MAC Address is 0090.1a00.00e0 key 8
    Partner System Priority 0 System MAC Address is 0000.0000.0000 key 0
    QoS parameter: vlan 1500000
    Attached QoS profile: eth1
    Member-interface FastEthernet11/2 is Up
    (LACP disabled, state collecting/distributing)
    Member-interface FastEthernet11/3 is Down
    (LACP disabled, state waiting)
    Member-interface FastEthernet11/4 is Up
    (LACP disabled, state collecting/distributing)

#### Meaning

Table 1 lists the related show interfaces lag memberscommand output fields.

Table 1: show interfaces lag members Output Fields

Field Name | Field Description
--- | ---
Lag | Name of the LAG bundle
QoS parameter | QoS parameter instance at the displayed interface
Attached QoS profile | QoS profile attachment at the displayed interface

#### Related Topics

- Configuring the Scheduler Hierarchy for Hashed Load Balancing in 802.3ad Link Aggregation Groups
- Configuring the Scheduler Hierarchy for Subscriber Load Balancing in 802.3ad Link Aggregation Groups
- Creating Parameter Instances
- For more information about other fields displayed with this command, see the JunosE Physical Layer Configuration Guide
- show interfaces lag members

#### Published: 2010-06-30

Help
|
My Account
|
Log Out