Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass fragmentation

# Configuring Fragmentation on Multiclass MLPPP Interfaces

You can configure fragmentation on a multiclass MLPPP interface with the same fragment size as that of the MLPPP interface.

Before you configure fragmentation on the multiclass MLPPP interface:

- Ensure that fragmentation is enabled on the MLPPP interface.

  See Configuring MLPPP Fragmentation and Reassembly in Chapter 8, Configuring Multilink PPP.

To configure fragmentation on a multiclass MLPPP interface:

- Specify the QoS traffic classes to be fragmented.

  - To configure fragmentation on multilink classes in a dynamic profile:

    host1(config-profile)#ppp multilink multiclass fragmentation best-effort voice otherData video

  - To configure fragmentation on multilink classes in a static MLPPP interface:

    host1(config-if)#ppp multilink multiclass fragmentation best-effort voice otherData video

  The order of the QoS traffic classes does not affect the execution of the command.

  | Note: You must include the best-effort traffic class in the ppp multilink multiclass fragmentation command, or the command fails.

#### Related Topics

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass fragmentation

#### Published: 2010-07-07

Help
|
My Account
|
Log Out