Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# tunnel mpls bandwidth

#### Syntax

tunnel mpls [ traffic-eng ] bandwidth bandwidth

no tunnel mpls [ traffic-eng ] bandwidth

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the bandwidth required for the tunnel. The no version removes the bandwidth constraint from the tunnel.

When the bandwidth constraint is configured, MPLS automatically creates and attaches a QoS profile to the tunnel to enforce the bandwidth reservation. The QoS profile creates a scheduler node at the LSP level, with a scheduler profile that has an assured rate corresponding to the reserved bandwidth. The QoS profile also creates queues above the scheduler node so that traffic of a particular class will be subject to the scheduler node. If no queue are created at the LSP level for a particular class, the traffic of that class enters that class's queue at a lower level, bypassing the bandwidth reservation enforcement.

#### Options

- traffic-eng—Specifies optional keyword for compatibility with non–E Series implementations
- bandwidth—Amount of bandwidth required for the tunnel in kilobits per second, in the range 0–4294967295; default value is 0

#### Mode

Interface Configuration, Tunnel Profile Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out