Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show ipv6 tunnel-route

#### Syntax

show ipv6 tunnel-route [ vrf vrfName ] [ ipv6Address [ detail ] | ipv6Prefix [ detail ] ]
[ all ] [ protocol ] [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
vrf keyword and vrfName variable added in JunosE Release 7.2.0.

#### Description

Displays current state of the IPv6 tunnel routing table.

#### Options

- vrfName—Name of the VRF
- ipv6Address—IPv6 address
- ipv6Prefix—Prefix of prefix list entry; in the format IPv6baseaddress / length; for example, 1::1/32
- detail—Displays detailed information about the specific route
- all—Displays all routes in the IPv6 tunnel routing table inserted from all protocols, not just the best routes
- protocol—The following protocols for which you want to display the best route or all routes in the tunnel routing table; no routes are displayed if routes for the specified protocol are not present in the tunnel routing table

  | Note: Other protocol options are available in the CLI, but they are not applicable to the tunnel routing table.

  - bgp-tunnel—Displays the BGP tunnel routes in the tunnel routing table
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out