Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- OAM Discovery Feature
- Configuring 802.3ah OAM Link-Fault Management
- ethernet oam lfm mode

# ethernet oam lfm pdu-lost-threshold

#### Syntax

[ no ] ethernet oam lfm pdu-lost-threshold pduLostPackets

#### Release Information

Command introduced in JunosE Release 11.1.0.

#### Description

Configures the number of OAM protocol data units (PDUs) that a local OAM client can fail to receive from a remote peer before a link-fault event is triggered. The no version removes the configured threshold for PDUs that can be missed from a remote peer before the generation of a link-fault event.

#### Options

- pduLostPackets—Number of expected OAM packets from the remote peer that the local OAM client can miss before a link-fault event is triggered; a number in the range 3–10; default value is 5

#### Mode

Interface Configuration

#### Related Topics

- OAM Discovery Feature
- Configuring 802.3ah OAM Link-Fault Management
- ethernet oam lfm mode

#### Published: 2010-07-19

Help
|
My Account
|
Log Out