Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Attaching a QoS Profile to an Interface
- Enabling Default Subscriber Load Balancing for 802.3ad Link Aggregation Groups

# qos-port-type-profile

#### Syntax

qos-port-type-profile typeOfInterface qos-profile qosProfileName

#### Release Information

Command introduced before JunosE Release 7.1.0.
lag keyword added in JunosE Release 8.1.0.

#### Description

Associates a QoS profile with all the ports of a given interface type. There is no no version.

#### Options

- typeOfInterface—One of the following interface types to be associated with the QoS port-type profile; atm, ethernet, lag, serial, server-port
- qosProfileName—Name of the QoS profile

#### Mode

Global Configuration

#### Related Topics

- Attaching a QoS Profile to an Interface
- Enabling Default Subscriber Load Balancing for 802.3ad Link Aggregation Groups

#### Published: 2010-07-13

Help
|
My Account
|
Log Out