Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Monitoring L2VPN Interfaces in the JunosE BGP and MPLS Configuration Guide

# show l2vpn interface

#### Syntax

show l2vpn interface [ instance l2VpnName | interfaceType interfaceSpecifier ] [ detail ]
[ filter ]

#### Release Information

Command introduced in JunosE Release 8.1.0.

#### Description

Displays information about layer 2 interfaces configured to be members of VPWS L2VPNs in the current VR: all layer 2 interfaces in the specified VPWS instance, all layer 2 interfaces in all VPWS instances, or a specific layer 2 interface.

#### Options

- l2VpnName—Name of the VPWS instance
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- detail—Displays detailed information
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring L2VPN Interfaces in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-07-14

Help
|
My Account
|
Log Out