Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Grouping ICR Subscribers Based on S-VLAN IDs
- Grouping ICR Subscribers Based on VLAN IDs
- Configuring an ICR Partition

# ip vrrp icr-partition group

#### Syntax

ip vrrp vrid icr-partition group partitionGroupingType

#### Release Information

Command introduced in JunosE Release 10.3.0.

#### Description

Configures the ICR partition to use either S-VLAN-based grouping or VLAN-based grouping for subscribers. If you specify VLAN as the grouping type or partition type, the ICR partition consists of single-tagged VLAN-based subinterfaces. By default, the ICR partition uses S-VLAN-based grouping. There is no no version.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- partitionGroupingType—One of the following partition types:
  - svlan—Configures the ICR partition to use double-tagged S-VLAN based subinterfaces.
  - vlan—Configures the ICR partition to use single-tagged VLAN based subinterfaces.

#### Mode

Interface Configuration, Subinterface Configuration

#### Related Topics

- Grouping ICR Subscribers Based on S-VLAN IDs
- Grouping ICR Subscribers Based on VLAN IDs
- Configuring an ICR Partition

#### Published: 2010-07-19

Help
|
My Account
|
Log Out