[ Contents] [ Prev] [ Next] [ Report an Error]

> Table 1: End-of-Life Modules for ERX Routers

> Combination Name | Line Module Label | I/O Module Label | First JUNOSe Support | Last JUNOSe Support | Page
> --- | --- | --- | --- | --- | ---
> CE1 |
> CE1 | CE1 | CE1 FULL I/O | 1.1.0 | 7.3.x | View
> Channelized T1 |  |  |  |  |
> CT1 | CT1 | CT1 FULL I/O | 1.1.0 | 7.3.x | View
> Channelized T3 |
> CT3 (3 ports) | CT3 | CT3/T3 I/O | 1.0.0 | 7.0.x | View
> E3 |
> E3 ATM | E3 ATM | E3 I/O | 1.1.0 | 7.1.x | View
> E3 Frame (3 ports) | E3 FRAME | E3 I/O | 1.1.0 | 7.0.x | View
> Fast Ethernet |
> FE-2 (2 ports) | FE-2 | FE-2 I/O | 1.3.0 | 7.0.x | View
> FE-8 (8 ports) (128 MB) Only line module is EOL. | GE/FE | FE-8 I/O | 2.0.0 | 5.2.x | View
> Gigabit Ethernet (1–port) |
> GE 1000Base-LH (128 MB) Only line module is EOL. | GE/FE | GE I/O SFP | 2.0.0 | 5.2.x | View
> GE 1000Base-SX (128 MB) Only line module is EOL. | GE/FE | GE I/O SFP | 2.0.0 | 5.2.x | View
> GE 1000Base-ZX (128 MB) Only line module is EOL. | GE/FE | GE I/O SFP | 2.0.0 | 5.2.x | View
> HSSI
> HSSI | HSSI-3F | HSSI-3 I/O | 3.1.0 | 7.3.x | View
> OC3/STM1 |
> OC3 (dual-port) multimode | OC3 | OC3 I/O MULTI MODE | 1.0.0 | 4.1.x | View
> OC3 (dual-port) single-mode | OC3 | OC3 I/O SINGLE MODE | 1.0.0 | 4.1.x | View
> OC3/STM1 ATM |
> OC3/STM1 ATM multimode without APS/MSP redundancy (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | OC3-4 I/O MULTI MODE | 2.0.0 | 5.2.x | View
> OC3/STM1 ATM single-mode intermediate reach without APS/MSP redundancy (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | OC3-4 I/O SINGLE MODE | 2.0.0 | 5.2.x | View
> OC3/STM1 ATM single-mode long reach without APS/MSP redundancy (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | OC3-4 I/O LONG HAUL | 2.0.0 | 5.2.x | View
> OC12/STM4 ATM |
> OC12/STM4 ATM multimode without APS/MSP redundancy (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | OC12 STM4 I/O MULTI MODE | 2.0.0 | 5.2.x | View
> OC12/STM4 ATM single-mode intermediate reach without APS/MSP redundancy (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | OC12 STM4 I/O SINGLE MODE | 2.0.0 | 5.2.x | View
> OC12/STM4 ATM single-mode long reach without APS/MSP redundancy (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | OC12 STM4 I/O LONG HAUL | 2.0.0 | 5.2.x | View
> SRPs |
> SRP-5G (512 MB) | SRP-5G | SRP I/O | 1.0.0 | 5.2.x | View
> SRP-5G+ (512 MB) | SRP-5G+ | SRP I/O | 3.0.2 | 8.0.x | View
> SRP-10G (512 MB) | SRP-10G | SRP I/O | 1.1.0 | 5.2.x | View
> SRP-10G (1-GB memory) | SRP-10G | SRP I/O | 4.1.3, 5.0.4, 5.1.2, 5.2.0 | 8.0.x | View
> SRP-SE10G (512 MB) | SRP-SE10G | SRP-SE I/O | 5.1.0 | 7.1.x | View
> SRP-40G (512 MB) | SRP-40G | SRP I/O | 3.4.1 | 5.2.x | View
> SRP-40G PLUS (1 GB) | SRP-40G PLUS | SRP I/O | 4.0.0 | 7.1.x | View
> T3 |
> T3 ATM (3 ports) | T3 ATM | CT3/T3 I/O | 1.1.0 | 7.0.x | View
> T3 ATM (4 ports) (128 MB) Only line module is EOL. | OCx/STMx ATM or OCx/STMx /DS3-ATM | 4xDS3 ATM I/O | 4.1.0 | 5.2.x | View
> T3 Frame (3 ports) | T3 FRAME | CT3/T3 I/O | 1.1.0 | 7.0.x | View
> Tunnel Service Module (TSM) |
> TSM | TUNNEL SERVICE | No I/O module | 3.0.2 | 8.0.x | View
> X.21/V.35
> X.21/V.35 | X.21/V.35 | X.21/V.35 I/O | 2.10.1, 3.3.2 | 7.3.x | View

[ Contents] [ Prev] [ Next] [ Report an Error]