# Monitoring the Packet Mirroring Configuration of IP Interfaces

#### Purpose

Display CLI-based packet mirroring configuration information for a specific interface or for all interfaces on which mirroring is enabled.

| Note: This command is deprecated and might be removed completely in a future release. The function provided by this command has been replaced by the show secure policy-list command.

#### Action

To display information about a specific interface or for all interfaces:

    host1#show ip mirror interface atm 5/0.1

        Interface          Analyzer Port      Analyzer next-hop
    ------------------- ------------------- ---------------------
    ATM5/0.1             FastEthernet3/0       192.168.1.1

#### Meaning

Table 62 lists the show ip mirror interface command output fields.

Table 62: show ip mirror interface Output Fields

Field Name | Field Description
--- | ---
Interface | Interface being mirrored
Analyzer Port | Interface to which the mirrored traffic is sent, and that then sends the traffic to the analyzer device
Analyzer next-hop | IP address of the next hop to the analyzer device; displayed when the analyzer interface is a shared medium

#### Related Topics

- show ip mirror interface