Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show l2tp received-disconnect-cause-summary

#### Syntax

show l2tp received-disconnect-cause-summary [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays aggregate summary statistics for all information received by an LAC from an LNS about the cause of an L2TP session disconnection. The LAC receives this information from the LNS by means of a PPP Disconnect Cause Code attribute value pair (AVP) included in an L2TP Call-Disconnect-Notify (CDN) message.

#### Options

- filter—See Filtering show Commands

#### Mode

Privileged Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out