Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring Routing in the Core for VPLS in the JunosE BGP and MPLS Configuration Guide

# router ospf

#### Syntax

[ no ] router ospf processId [ vrf vrfName ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an OSPF routing process. The no version disables an OSPF routing process.

#### Options

- processId—Number, in the range 1–65535, that identifies the OSPF process
- vrfName—Name of the VRF; string of 1–32 alphanumeric characters; available only in virtual router context, not VRF context

#### Mode

Global Configuration

#### Related Topics

- Configuring Routing in the Core for VPLS in the JunosE BGP and MPLS Configuration Guide

#### Published: 2010-07-14

Help
|
My Account
|
Log Out