Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Creating or Modifying Classifier Control Lists for VLAN Policy Lists

# vlan classifier-list

#### Syntax

vlan classifier-list classifierName
[ traffic-class className ] [ color { green | yellow | red } ]
[ user-packet-class userPacketClassValue ] [ user-priority userPriorityValue ]

no vlan classifier-list classifierName [ classifierNumber ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Creates or modifies a VLAN classifier control list. The no version deletes the classifier control list.

#### Options

- classifierName—Name of a classifier list entry
- className—Name of a traffic class; the router supports up to eight traffic classes
- green—Matches packet color to green, indicating a low drop preference
- yellow—Matches packet color to yellow, indicating a medium drop preference
- red—Matches packet color to red, indicating a high drop preference
- userPacketClassValue—Value of the user packet class in the range 0–15
- userPriorityValue—Value of the user priority bits in the range 0–7
- classifierNumber—Index of the classifier control list entry to be deleted; an integer in the range 1–10000

#### Mode

Global Configuration

#### Related Topics

- Creating or Modifying Classifier Control Lists for VLAN Policy Lists

#### Published: 2010-07-14

Help
|
My Account
|
Log Out