Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Configuring CLI-Based Mirroring

# mirror analyzer-ip-address

#### Syntax

mirror analyzer-ip-address analyzerIpAddress analyzer-virtual-router vrName
[ analyzer-udp-port udpPort [ mirror-identifier mirrorId
[ session-identifier sessionId ] ] ]

no mirror

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the mirror action for a classifier group in a secure IP or L2TP policy list. The no version deletes the mirror rule.

#### Options

- analyzerIpAddress—IP address of the analyzer
- vrName—Name of the virtual router where the analyzer interface is configured
- udpPort—UDP port of the analyzer; required for L2TP packet mirror rules
- mirrorId—Mirror identifier
- sessionId—Session identifier

#### Mode

Classifier-Group Configuration

#### Related Topics

- Configuring CLI-Based Mirroring

#### Published: 2010-07-19

Help
|
My Account
|
Log Out