Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Monitoring QoS Parameter Instances

# show qos-parameter

#### Syntax

To display settings for a specific parameter instance with references:

show qos-parameter [ qosParameterInstanceName ] references [ brief | full ] [ filter ]

To display references globally:

show qos-parameter [ qosParameterInstanceName ] references global
[ qosParameterInstanceName ] [ brief | full ] [ filter ]

To display references for interfaces:

show qos-parameter [ qosParameterInstanceName ] references [ interface interfaceType interfaceSpecifier [ atmVpi | s-vlanIdValue ] ] [ explicit ] [ brief | full ]
[ filter ]

To display references for L2TP sessions:

show qos-parameter [ qosParameterInstanceName ] references lt2p session sessionName [ explicit ] [ filter ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
full keyword added in JunosE Release 7.2.0.

#### Description

Displays QoS parameter instance settings for QoS clients.

#### Options

- qosParameterInstanceName—Name of the parameter instance
- references—Displays interfaces that reference this parameter instance
- global—Displays information about global parameter instances
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- sessionName —Name of the L2TP session
- brief—Displays information in a condensed format
- full—Displays information in expanded format
- explicit—Displays parameter instances only on the specified interface and not parameter instances stacked above the interface
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

#### Related Topics

- Monitoring QoS Parameter Instances

#### Published: 2010-07-14

Help
|
My Account
|
Log Out