# frame-relay lmi-type

#### Syntax

frame-relay lmi-type type

no frame-relay lmi-type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Selects the LMI type. The no version restores the default value.

#### Options

- type—One of the following types:
  - ansi—ANSI T1.617 Annex D
  - cisco—Original Group of Four specification developed by DEC, Northern Telecom, Stratacom, and Cisco
  - q933a—ITU-T Q.933 Annex A
  - none—No management interface is used

#### Mode

Interface Configuration

#### Related Topics

- Configuring Frame Relay Layer 2 Services in the JunosE BGP and MPLS Configuration Guide