Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# mode

#### Syntax

mode { file-system-synchronization | high-availability }

no mode

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables high availability mode (hitless SRP switchover) operation. The no version returns high availability mode operation to its default (file-system-synchronization).

#### Options

- file-system-synchronization—Uses file synchronization to keep the configuration of the standby SRP coordinated with the configuration of the active SRP
- high-availability—Uses mirroring to keep the configuration and state of the standby SRP coordinated with the configuration and state of the active SRP

#### Mode

Redundancy Configuration

#### Published: 2010-07-19

Help
|
My Account
|
Log Out