Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# tunnel mpls no-route retry-time

#### Syntax

tunnel mpls no-route retry-time retryTime

no tunnel mpls no-route retry-time

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies for a particular tunnel the interval in seconds between attempts to set up an LSP for RSVP-TE after a failure due to no available route. The no version restores the default value, 5 seconds.

#### Options

- retryTime—Number of seconds in the range 1–60

#### Mode

Interface Configuration, Tunnel Profile Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out