Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# radius override nas-ip-addr tunnel-client-endpoint

#### Syntax

radius override nas-ip-addr tunnel-client-endpoint

no radius override nas-ip-addr

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the RADIUS client (LNS) to override the standard use of the NAS-IP-Address [4] RADIUS attribute and instead use the tunnel-client-endpoint (LAC) IP address. The no version restores the default address.

#### Mode

Global Configuration

#### Published: 2010-07-13

Help
|
My Account
|
Log Out