Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show l2tp tunnel

#### Syntax

show l2tp tunnel [ detail ] [ state { adminState | ifOperStatus |
failover-resync failoverResyncMode } ]
[ l2tpName | [ virtual-router vrName ] ip ipAddress [ l2tpNameNoDest ] ] [ filter ]

To display summary information:

show l2tp tunnel summary [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
failover-resync keyword and failoverResyncMode variable added in JunosE Release 9.0.0.

#### Description

Displays detailed information about the configured and operational status of selected L2TP tunnels or summary information for all L2TP tunnels.

#### Options

- detail—Provides complete information about the specified sessions, including the L2TP host profile name
- adminState—Displays information about tunnels only with the specified effective administrative state
  - enabled—Effective administrative state is disabled
  - disabled—Effective administrative state is enabled
  - drain—Effective administrative state is drain
- ifOperStatus—Displays information about tunnels only with the specified operational state
  - up—Operational state is up
  - down—Operational state is down
  - lower-down— Operational state is lower down
  - not-present—Operational state is not-present
- failoverResyncMode—Displays information about tunnels that use the specified failover resynchronization mode:
  - disable—Peer failover resynchronization is disabled
  - failover-protocol—Uses the L2TP failover protocol method
  - failover-protocol-fallback-to-silent-failover—Uses the L2TP failover protocol method; however, if the peer does not support this method, the silent failover method is used
  - not-configured—Uses the global failover method because peer failover resynchronization is not configured for L2TP host profiles and AAA domain map tunnels
  - silent-failover—Uses the L2TP silent failover method
- l2tpName—Tunnel name
- vrName—Name of the virtual router on which the tunnel exists
- ipAddress—IP address
- l2tpNameNoDest—Tunnel name
- filter—See Filtering show Commands
- summary—Displays the configured and operational status of all L2TP tunnels

#### Mode

Privileged Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out