Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Monitoring the Packet Mirroring Configuration of IP Interfaces

# show ip mirror interface

#### Syntax

show ip mirror interface [ vrf vrfName ] [ interfaceType interfaceSpecifier ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays information about the interface mirroring configuration of all interfaces, or for a specific interface on which mirroring is enabled.

| Note: This command is deprecated and might be removed completely in a future release. The function provided by this command has been replaced by the show secure policy-list command.

#### Options

- vrfName—Name of the VRF
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers

#### Mode

Privileged Exec

#### Related Topics

- Monitoring the Packet Mirroring Configuration of IP Interfaces

#### Published: 2010-07-14

Help
|
My Account
|
Log Out