Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# show ppp interface

#### Syntax

show ppp interface [ interfaceType interfaceSpecifier ]
[ full | { dataRestriction }* [ protocolRestriction ]* ] [ state stateRestriction ]
[ delta ] [ filter ]

For multilinked PPP interfaces, the following options are additionally available:

show ppp interface mlppp [ interfaceSpecifier ] members [ filter ]

show ppp interface mlppp links [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
eap keyword added in JunosE Release 7.3.0.

#### Description

Displays information about the PPP interface type that you specify.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- full—Displays configuration, status, and statistics information for the interface, including information specific to LCP, IPCP, OSINLCP, MPLSCP, PAP, and CHAP; equivalent to specifying config status statistics
- dataRestriction—One or more of the following keywords; you can repeat a keyword without effect
  - config—Displays information about the PPP interface configuration
  - status—Displays information about the PPP interface operational status
  - statistics—Displays information about the PPP interface statistics
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- protocolRestriction—One or more of the following keywords
  - eap—Displays EAP-specific information
  - lcp—Displays LCP-specific information
  - ip—Displays IPCP-specific information
  - ipv6—Displays IPv6CP-specific information
  - osi—Displays OSINLCP-specific information
  - mpls—Displays MPLSCP-specific information
  - pap—Displays PAP-specific information
  - chap—Displays CHAP-specific information
- stateRestriction—Information is displayed only for interfaces in one of the following specified states:
  - open—Interface is administratively enabled, meaning that the no ppp shutdown command is operational
  - closed—Interface is administratively disabled, meaning that the ppp shutdown command is operational
  - up—Interface on which the LCP has been negotiated
  - down—Interface on which the LCP has not been negotiated, the negotiations have failed, or the connection has been ended
  - lower-layer-down—Interface that is not up and is waiting for the lower layer to come up to initiate negotiations for LCP
  - not-present—Interface that is not present because the hardware is not available. When the interface is in this state, no detailed information is available.
  - passive—Interface with the operational status passive
  - tunneled—Tunneled PPP interfaces
  - no-ip—Interface on which IPCP is not configured
  - ip-open—Interface on which IPCP is administratively enabled, meaning that the no ppp shutdown ip command is operational
  - ip-closed—Interface on which IPCP is administratively disabled, meaning that the ppp shutdown ip command is operational
  - ip-up—Interface on which the IPCP has been negotiated
  - ip-down—Interface on which the IPCP has not been negotiated, the negotiations failed, or the connection has been ended
  - no-ipv6—Interface on which IPv6CP is not configured
  - ipv6-open—Interface on which IPv6CP is administratively enabled, meaning that the no ppp shutdown ipv6 command is operational
  - ipv6-closed—Interface on which IPv6CP is administratively disabled, meaning that the ppp shutdown ipv6 command is operational
  - ipv6-up—Interface on which the IPv6CP has been negotiated
  - ipv6-down—Interface on which the IPv6CP has not been negotiated, the negotiations failed, or the connection has been ended
  - no-osi—Interface on which OSINLCP is not configured
  - osi-open—Interface on which OSINLCP is administratively enabled, meaning that the no ppp shutdown osi command is operational
  - osi-closed—Interface on which OSINLCP is administratively disabled, meaning that the ppp shutdown osi command is operational
  - osi-up—Interface on which the OSINLCP has been negotiated
  - osi-down—Interface on which the OSINLCP has not been negotiated, the negotiations failed, or the connection has been ended
  - no-mpls—Interface on which MPLSCP is not configured
  - mpls-open—Interface on which MPLSCP is administratively enabled, meaning that the no ppp shutdown mpls command is operational
  - mpls-closed—Interface on which MPLSCP is administratively disabled, meaning that the ppp shutdown mpls command is operational
  - mpls-up—Interface on which the MPLSCP has been negotiated
  - mpls-down—Interface on which the MPLSCP has not been negotiated, the negotiations failed, or the connection has been ended
- delta—Displays baselined statistics
- filter—See Filtering show Commands
- members—Lists all MLPPP member links, or only those for a specified MLPPP bundle
- links—Lists all MLPPP encapsulated links, regardless of whether the links are members of an MLPPP bundle

#### Mode

Privileged Exec, User Exec

#### Published: 2010-07-14

Help
|
My Account
|
Log Out