# Index

Symbols A B C D E F G H I J K L M N O P R S T U V W X

Symbols

> 10-Gigabit Ethernet interfaces
>   for E120 and E320 routers 1, 2, 3
> 10-Gigabit Ethernet modules
>   specifying an interface 1, 2, 3, 4, 5, 6
> 802.3ad link aggregation
>   E120 and E320 routers 1
> 802.3ah link-fault management
>   E120 and E320 routers 1, 2
> 802.3ah OAM link-fault management See Ethernet OAM link-fault management

A

> AAA (authentication, authorization, accounting)
>   sending ATM interface descriptions to 1
> aaa commands
>   aaa domain-map 1
>   aaa tunnel calling-number-format 1
>   aaa tunnel calling-number-format fallback 1
> AAL (ATM Adaptation Layer) 1
> AAL5 encapsulation
>   functions of access nodes 1
>   interworking function 1, 2
> AAL5 encapsulation types 1
> AC-Cookie tag, PPPoE 1
> AC-Name tag, PPPoE 1
> access nodes
>   as Ethernet switches 1
>   digital subscriber lines (DSL) and 1
>   in Ethernet aggregation networks, overview 1
>   interworking functions 1
> accounting statistics
>   terminated PPP session 1
> active discovery mode
>   and OAM link-fault management 1
>   configuration on
>     provider edge devices 1
>   functions of 1
>   performance variables
>     responding to 1
>     retrieval of 1
>   starting remote loopback
>     by the local entity 1
>   triggering the discovery process 1
> address ranges
>   VPI/VCI 1, 2
> Agent-Circuit-Id
>   format of
>     configuration scenario for encapsulation lockout, IWF PPPoE sessions 1
> Agent-Circuit-Id DSL Forum VSA
>   usage in dynamic encapsulation lockout
>     for IWF PPPoE sessions 1
> agent-circuit-identifier and dynamic VLAN subinterfaces 1, 2
> Agent-Remote-Id DSL Forum VSA
>   usage in dynamic encapsulation lockout
>     for IWF PPPoE sessions 1
> aggregating T1 or E1 lines 1, 2
> aggregation, Ethernet link 1
> AIS (alarm indication signal) cells 1, 2
> alarm indication signal cells. See AIS cells
> ARP (Address Resolution Protocol) table 1
> arp commands
>   arp 1
> ARP, Inverse 1
> Asynchronous Transfer Mode. See ATM
> ATM (Asynchronous Transfer Mode) 1, 2, See also OAM, ATM
>   AAL 1
>   AIS cells, handling 1
>   ATM passthrough 1
>   cable lengths 1
>   CAC 1
>   CC cells 1
>   cell scrambling payload 1
>   configuring 1, 2, 3, 4
>   dynamic interfaces 1
>   E120 and E320 routers 1, 2, 3, 4, 5, 6, 7, 8, 9
>   E320 routers 1, 2
>   fault management 1
>   ILMI 1
>   interface description 1
>   loopback cells, handling 1, 2
>   Martini encapsulation 1
>   module capabilities (statistics) 1
>   monitoring 1
>   OAM 1
>   oversubscription for dynamic interfaces 1, 2
>   overview 1
>   ping
>     configuring 1
>     overview 1
>   platform considerations 1
>   PVCs
>     configuring 1, 2
>     configuring individual parameters for 1
>     defining 1
>   RDI cells, handling 1
>   testing 1
>   VC classes 1
>   VC integrity 1
>   VCC-layer connectivity verification 1
> ATM 1483 subinterfaces, dynamic
>   assigning VC classes to 1, 2, 3
>   benefits of using 1
>   bulk configuration of VC ranges 1
>   changing VC subranges 1, 2
>   configuring 1
>   creating static ATM interfaces inVC subranges 1, 2
>   exporting descriptions 1
>   monitoring 1
>   overriding base profile assignments 1, 2
>   oversubscription 1, 2
>   overview 1
>   profiles for 1
>   restarting LCP negotiations for PPPoA clients 1
> atm aal5 commands
>   atm aal5 description 1
>   atm aal5 shutdown 1
>   atm aal5 snmp link-status 1
> ATM Adaptation Layer. See AAL
> atm atm1483 commands
>   atm atm1483 advisory-rx-speed 1, 2, 3, 4
>   atm atm1483 auto-configure 1
>   atm atm1483 description 1, 2, 3
>   atm atm1483 export-subinterface-description 1
>   atm atm1483 mtu 1
>   atm atm1483 profile 1
>   atm atm1483 shutdown 1
>   atm atm1483 snmp trap link-status 1
>   atm atm1483 subscriber 1, 2
> atm commands 1, See also show atm commands
>   atm auto-configuration 1
>   atm bulk-config 1, 2, 3, 4
>   atm bulk-config modify 1
>   atm bulk-config shutdown 1
>   atm cac 1
>   atm class-vc 1
>   atm clock internal 1
>   atm description 1
>   atm framing 1, 2
>   atm ilmi-enable 1
>   atm ilmi-keepalive 1, 2, 3
>   atm lbo 1, 2
>   atm oam 1
>   atm oam flush 1, 2, 3
>   atm oam loopback-location 1
>   atm pvc 1, 2, 3, 4, 5, 6, 7
>   atm shutdown 1
>   atm snmp trap link-status 1
>   atm sonet 1
>   atm sonet stm-1 1
>   atm uni-version 1, 2
>   atm vc-per-vp 1, 2, 3
>   atm vp-description 1
>   atm vp-tunnel 1, 2
>   monitor atm vc 1
>   monitor atm vp 1
>   ping atm interface atm 1
> ATM VC Configuration mode 1
> ATM virtual circuit (VC) 1
> ATM-to-Ethernet interworking
>   arrival of a PPPoA session at the DSLAM
>     and conversion into a PPPoE session at the DSLAM 1
>   configuration examples for
>     1:1 association between DSLAM and B-RAS 1
>     N:1 association between DSLAMs and B-RAS 1
>   conversion from ATM to Ethernet
>     mapping method for tags 1
>   conversion from Ethernet to ATM
>     mapping method for tags 1
>   cross-connect
>     provision of Layer 2 switching 1
>   distinction between IWF and non-IWF PPPoE sessions
>     using the IWF PPPoE tag 1
>   method of mapping of ATM to Ethernet packets 1
>   overview 1
>   translation of ATM into Ethernet traffic 1
>   transmission of a PPPoE session
>     to the access concentrator 1
> authentication
>   EAP 1
>   MLPPP 1
>   PPP 1, 2, 3
>   subscribers on dynamic bridged Ethernet interfaces 1, 2, 3
> auto-configure commands
>   auto-configure 1, 2, 3, 4
>   auto-configure atm1483 1, 2
>   auto-configure vlan 1
> autodetection of dynamic interfaces 1, 2

B

> B-RAS application
>   authentication of PPPoE packets 1
>   IWF PPPoE sessions
>     multiple DSLAMs connected to an access concentrator 1
>     one DSLAM connected to an access concentrator 1
>   usage of the IWF PPPoE tag
>     in identifying IWF sessions 1
> B-RAS applications, with PPP sessions 1
> B-RAS device
>   operation for
>     interworked PPPoA sessions 1
>     interworked PPPoE over ATM sessions 1
> bandwidth
>   SONET/SDH 1
> base profiles
>   VLAN subinterfaces 1
> baseline commands
>   baseline atm 1
>   baseline atm vp interface 1
>   baseline bridge 1
>   baseline bridge interface 1
>   baseline frame-relay 1
>   baseline frame-relay interface 1
>   baseline frame-relay multilinkinterface 1
>   baseline hdlc interface serial 1
>   baseline interface atm 1
>   baseline interface pos 1
>   baseline ppp (MLPPP) 1
>   baseline ppp interface 1
>   baseline pppoe interface 1
> bridge commands 1, See also clear bridge commands; show bridge commands; subscriber policy commands
>   bridge 1
>   bridge acquire 1
>   bridge address 1
>   bridge aging time 1
>   bridge crb 1
>   bridge learn 1
>   bridge route 1
>   bridge snmp-trap link-status 1
>   bridge subscriber-policy 1
>   bridge-group 1
> bridge groups
>   configuring optional attributes 1
>   creating 1
>   defined 1
>   monitoring 1
> bridge interfaces
>   configuring 1
>   defined 1
>   monitoring 1
>   supported configurations 1
>   types of 1
> bridge1483 commands
>   bridge1483 mtu 1
>   bridge1483 service-profile 1
> bridged Ethernet dynamic interfaces 1
>   authenticating subscribers 1, 2, 3
>   profile characteristics 1
> bridged Ethernet static interfaces 1
>   application 1
>   backward compatible configuration 1
>   configuring 1
>   configuring for terminated traffic 1
>   configuring MTU size 1
>   configuring S-VLANs 1
>   configuring VLANs 1
>   E120 and E320 routers 1
>   MAC address validation 1
>   monitoring 1
>   platform considerations 1
>   terminating and routing traffic 1
>   VLAN and S-VLAN support 1
> bridged IP
>   configuring 1
>   E120 and E320 routers 1
>   overview 1
>   platform considerations 1
> bridging, transparent
>   concurrent routing and bridging 1, 2
>   configuration examples
>     bridged Ethernet 1
>     VLANs 1
>   configuration tasks 1
>   configuring
>     bridge groups and bridge interfaces 1, 2
>     optional bridge group attributes 1
>     routing 1
>     subscriber policies 1
>   creating bridge groups 1
>   E120 and E320 routers 1
>   MAC addresses 1, 2
>   monitoring 1
>   overview 1
>   platform considerations 1
>   prerequisites 1
>   references 1
>   setting statistics baselines 1
>   subscriber policies 1
>   unsupported features 1
> broadcast command 1
> bulk configuration of VC ranges 1
>   assigning VC classes 1, 2, 3
>   oversubscription 1, 2
>   restarting LCP negotiations for PPPoA clients 1
>   with CAC 1, 2
> bulk configuration of VLAN ranges 1
> bundle
>   MLFR 1, 2
>   MLPPP 1, 2

C

> C-VLAN tags
>   virtual path identifier (VPI) mapping to
>     in ATM-to-Ethernet conversion 1
> cable length
>   ATM interfaces 1
> CAC (connection admission control) for ATM
>   configuring 1, 2
>   overview 1
>   with bulk configuration 1, 2
> Calling Number AVP
>   descriptive format configuration 1
>   format configuration with agent ID suboptions 1
> cbr command 1, 2
> CE-side load balancing 1
> CE1 line modules
>   MLPPP features 1
> cells
>   AIS 1, 2
>   ATM 1
>   F4 OAM 1
>   fault management 1
>   handling of ATM loopback 1
>   loopback 1
>   RDI 1, 2
> Challenge Handshake Authentication Protocol. See CHAP
> channelized T1 interfaces
>   MLPPP features 1
> channelized T3 interfaces
>   end-to-end fragmentation and reassembly 1
>   MLPPP features 1
> CHAP (Challenge Handshake Authentication Protocol) 1
> circuit ID, capturing for PPPoE
>   configuring 1
>   dsl-forum-1 format and examples 1, 2
>   formatting 1, 2
>   monitoring 1
>   overview 1
>   sending to RADIUS or L2TP 1, 2
>   troubleshooting 1
>   using in profiles 1, 2
> Cisco HDLC
>   configuring 1
>   E120 and E320 routers 1
>   error frames 1
>   framing 1
>   line modules supported 1
>   monitoring 1
>   overview 1, 2
>   platform considerations 1
>   shutting down the interface 1
>   SLARP Address Resolution protocol 1
>   SLARP Keep-Alive protocol 1
>   SLARP keepalive interval 1
> class-int command 1, 2
> class-vc command 1
> classes, VC
>   assigning to
>     ATM major interfaces 1
>     dynamic ATM 1483 subinterfaces 1, 2, 3
>     PVCs 1
>     static ATM 1483 subinterfaces 1
>   benefits 1
>   configuring 1
>   examples
>     configuration 1
>     precedence levels 1
>   monitoring 1
>   overview 1
>   precedence levels 1
>   upgrade considerations 1
> clear bridge commands
>   clear bridge 1
>   clear bridge address 1
>   clear bridge interface 1
> clock commands
>   clock source
>     POS interfaces 1
> clock source, selecting
>   ATM interfaces 1
>   POS interfaces 1
> COCX-F3 line modules
>   MLPPP features 1
> cOCx/STMx interfaces
>   end-to-end fragmentation and reassembly 1
>   MLPPP features 1
> cold router restart
>   preservation of
>     settings for enabling and disabling remote loopback 1
> concurrent routing and bridging. See CRB
> configuration examples
>   ATM 1483 subinterfaces, dynamic 1
>   ATM VC classes 1, 2
>   bridged Ethernet, dynamic 1
>   bridged Ethernet, static 1
>   Cisco HDLC 1
>   IPoA, dynamic 1
>   MLFR 1
>   MLPPP, dynamic 1
>   MLPPP, static 1, 2
>   PPPoE, dynamic 1, 2
>   PPPoE, static 1, 2
>   profiles for dynamic interfaces 1
>   transparent bridging 1
>   VLAN subinterfaces, dynamic 1, 2
> configure file command 1
> configuring. See specific feature, product, or protocol
> connection admission control. See CAC for ATM
> connection types, ATM
>   multipoint 1
>   point-to-point 1
> control block
>   functions of
>     implementation of discovery process 1
>     rules management of received OAM PDUs from the parser 1
>     transmission of OAM PDUs to the multiplexer 1
>   interface between
>     OAM client and internal sublayer elements 1
> control PVCs, creating 1
> conventions
>   notice icons 1
>   text and syntax 1
> CRB (concurrent routing and bridging)
>   bridge crb command 1
>   bridge route command 1
>   configuring routing 1
>   defined 1
>   enabling 1
> crc command 1, 2
> creating an IP profile
>   tcp adjust-mss 1
> critical event
>   denoting an unspecified vendor-specific error condition 1
>   detection of error conditions
>     in the receive path of the link 1
>   influencing the link state
>     using the bit in the Flags field 1
>   OAM remote failure detection
>     notified constantly to the local entity 1
> critical event PDU
>   received from the remote peer
>     influencing the link state 1
>     OAM link monitoring 1
> CT3/T3-F0 line modules
>   MLPPP features 1
> customer support 1
>   contacting JTAC 1

D

> data communication equipment. See DCE
> data PVCs, creating 1
> data terminal equipment. See DTE
> data-link connection identifier. See DLCI
> DCE (data communication equipment)
>   configuring Frame Relay interface as 1, 2, 3
>   frame-relay lmi commands 1
>   show frame-relay lmi command 1, 2
> debugging PPP and PPPoE dynamic interfaces 1
> description, interface
>   ATM 1483 subinterfaces, exporting 1
>   ATM interfaces 1
>   ATM virtual paths 1
>   Frame Relay interfaces 1
>   POS interfaces 1, 2
>   sending to AAA 1
>   serial interfaces 1
> DHCP option 82 field 1
> DHCP relay
>   with bridged IP 1
> digital subscriber line access multiplexers. See DSLAMs
> discovery process See OAM discovery
> Discovery protocol with PPPoE 1
> DLCI (data-link connection identifier) 1, 2, 3
> documentation set
>   comments on 1
> ds3-scramble command 1
> DSL Forum VSAs
>   Agent-Circuit-Id
>     encapsulation type lockout 1
>   Agent-Remote-Id
>     encapsulation type lockout 1
>   as criteria for encaspulation type lockout 1
>   IWF-Session
>     dynamic encapsulation type lockout 1
>     PPPoE clients with duplicate MAC addresses 1
> dsl-forum-1 format for PPPoE remote circuit ID 1, 2
> DSLAM devices
>   IWF PPPoE sessions and
>     multiple DSLAMs connected to an access concentrator 1
>     single DSLAM connected to an access concentrator 1
> DSLAMs (digital subscriber line access multiplexers) 1
> DTE (data terminal equipment)
>   configuring Frame Relay interface as 1, 2, 3
>   frame-relay lmi command 1
>   show frame-relay lmi command 1, 2
> Duplicate event notification OAM PDUs
>   viewing 1
> duplicate protection
>   disabled for
>     IWF PPPoE sessions, method of processing 1
>     non-IWF PPPoE sessions, method of processing 1
>   enabled for
>     IWF PPPoE sessions, method of processing 1
>     non-IWF PPPoE sessions, method of processing 1
>   for an underlying interface
>     PPPoE logical interface activation and 1
>   for IWF PPPoE sessions
>     guidelines for configuring 1
>   of IWF PPPoE sessions
>     and access to network services 1
>     based on MAC addresses 1
>     guidelines for configuring 1
>     prevention of unauthorized access 1
>     scenarios of configuration 1
>   topologies for IWF PPPoE sessions
>     1:1 association between DSLAMs and the B-RAS application 1
>     N:1 association between DSLAMs and the B-RAS application 1
>   types of PPPoE sessions
>     with the IWF tag absent in PADR 1
>     with the IWF tag present in PADR 1
> dying gasp
>   cases in which it occurs 1
>   influencing the link state
>     using the bit in Flags field 1
>   OAM remote failure detection
>     using Flags field in Information PDUs 1
>   vendor-specific condition
>     notified constantly to the local entity 1
> dynamic encapsulation type lockout 1
>   based on DSL Forum VSAs
>     for IWF PPPoE sessions 1
>   benefits 1
>   configuring 1, 2, 3
>   criteria used in determining
>     for IWF PPPoE sessions 1
>   for IWF PPPoE sessions
>     guidelines for configuring 1
>     same as the behavior for non-IWF sessions, scenario 1
>     sample configuration scenario 1
>     single DSLAM connected to a B-RAS device 1
>     with DSL Forum VSAs not present in PADR 1
>   for PPPoE clients 1
>     clearing lockout condition 1
>     configuring 1
>     differences from PPPoE over static ATM 1
>     monitoring 1, 2, 3, 4, 5
>   grace period 1
>   guidelines 1
>   parameters used to perform
>     Agent-Circuit-Id 1
>     Agent-Remote-Id 1
>     MAC address 1
> Dynamic Host Configuration Protocol. See DHCP relay
> dynamic interfaces
>   ATM 1483 subinterfaces 1, 2
>   autodetection 1, 2
>   bridged Ethernet 1
>     authenticating subscribers 1, 2, 3
>   configuring from a profile 1, 2, 3
>   configuring from RADIUS 1
>   configuring IPoA 1
>   configuring Multiclass MLPPP 1
>   configuring PPP and PPPoE over ATM 1
>     restarting LCP negotiations 1
>   configuring PPPoE over static PPPoE 1
>     ATM interface columns 1
>     encapsulation type lockout 1
>     Ethernet and S-VLAN interface columns 1
>     Ethernet and VLAN interface columns 1
>     S-VLAN oversubscription 1, 2
>     static Ethernet interface columns 1
>   E120 and E320 routers 1, 2, 3
>   E320 routers 1, 2, 3
>   inserting dynamic IP routes intorouting table 1
>   monitoring 1, 2
>   oversubscription, ATM 1, 2
>   overview 1, 2
>   platform considerations 1, 2, 3
>   profiles, reassigning 1
>   RADIUS authentication 1, 2
>   troubleshooting 1
>   types supported 1, 2
>   VLAN subinterfaces 1
>   VLAN subinterfaces with agent-circuit-identifier information 1, 2

E

> E120 and E320 routers
>   10-Gigabit Ethernet interfaces 1, 2, 3
>   802.3ad link aggregation 1
>   802.3ah link-fault management 1, 2
>   ATM interfaces 1, 2, 3, 4, 5, 6, 7, 8, 9, 10
>   bridged IP interfaces 1
>   Cisco HDLC interfaces 1
>   dynamic interfaces 1, 2, 3
>   Gigabit Ethernet interfaces 1, 2, 3
>   POS interfaces 1, 2, 3, 4
>   PPP interfaces 1, 2
>   PPPoE interfaces 1, 2
>   transparent bridging 1
> e3-scramble command 1
> E320 routers
>   ATM interfaces 1
>   bridged Ethernet 1
>   dynamic interfaces 1, 2, 3
>   POS interfaces 1
>   PPP interfaces 1
> EAP (Extensible Authentication Protocol) 1
>   authentication methods 1
>   authentication negotiation 1
>   components 1
>   L2TP 1
>   limitations 1
>   MRU 1
>   MTU 1
>   performance 1
>   retransmission of packets 1
>   scalability 1
>   types 1
> ECMP (equal-cost multipath)
>   MLFR alternative to 1
>   MLPPP alternative to 1
> enable commands
>   enable 1
> enabling LMI 1
> enabling Multiclass MLPPP 1
> encapsulation commands
>   encapsulation 1, 2
>   encapsulation bridge1483 1, 2, 3
>   encapsulation frame-relay ietf 1, 2, 3
>   encapsulation hdlc 1
>   encapsulation mlframe-relay ietf 1
>   encapsulation mlppp 1, 2
>   encapsulation ppp 1, 2, 3, 4, 5, 6, 7
>   encapsulation pppoe 1, 2, 3
>   encapsulation vlan 1, 2, 3, 4
> encapsulation method
>   ATM interface 1, 2
>   Cisco HDLC interface 1
>   Frame Relay interface 1, 2, 3, 4, 5
> encapsulation type lockout. See dynamic encapsulation type lockout
> encapsulation, configuring for PVCs 1
> end-to-end fragmentation and reassembly, Frame Relay 1
> endpoint discriminator
>   MLPPP 1
> equal-cost multipath. See ECMP
> error frame seconds
>   configuring
>     high threshold 1
>     low threshold 1
>     window 1
> error frame seconds summary events
>   configuring
>     high threshold 1
>     low threshold 1
>     window 1
> error frames
>   Frame Relay 1
>   PPP 1
> Errored Frame Event TLV
>   in Event notification OAM PDUs
>     for tracking frame errors 1
> Errored Frame Seconds Summary Event TLV
>   in Event notification OAM PDUs
>     for tracking frame seconds summary errors 1
> Errored Symbol Period TLV
>   in Event notification OAM PDUs
>     for tracking symbol errors 1
> ES2-S1 Service IOA
>   MLPPP features 1
> Ethernet aggregation networks
>   access nodes in, overview 1
> Ethernet interfaces
>   CE-side load balancing 1
>   changing of the operational status
>     and generation of a link-fault event 1
>   commands 1, 2, See also show commands
>     interface fastEthernet 1
>     interface lag 1
>   failing over to the redundant link
>     when high threshold is exceeded 1
>   IEEE 802.1Q 1
>   IEEE 802.3ad 1
>   L2TP 1
>   link aggregation (LAG) 1
>   link-fault management
>     guidelines for configuring 1
>   monitoring 1, 2, 3
>   moving to the down state
>     when high threshold is exceeded 1
>   MPLS 1, 2
>   multinetting 1
>   OAM link-fault management 1
>   on SRP modules
>     and support for link-fault management 1
>   operational states
>     down state on OAM association tear-down 1
>     up state on OAM association rebuilding 1
>   PPPoE over S-VLANs 1
>   PPPoE over VLANs 1, 2
>   S-VLANs 1, 2
>   subnetwork attachment point (SNAP) 1
>   VLANs 1
> Ethernet link aggregation
>   CE-side load balancing 1
>   configuring 1
>   enabling CE-side load balancing 1
>   interoperation with OAM link-fault management
>     operation of 802.3ah below the LAG sublayer 1
>   IP interfaces
>     example 1
>   MPLS 1, 2
>   MPLS over VLAN 1
>   overview 1, 2
>   PPPoE subinterfaces 1
>     example 1
>   VLAN subinterfaces 1
>     example 1
> Ethernet link aggregation commands
>   interface lag 1
>   lacp 1
>   lacp port-priority 1
>   member-interface 1
>   minimum-links 1
>   pppoe subinterface lag 1
> Ethernet link redundancy
>   configuration models 1
>   configuring 1
>   link behavior 1
>   overview 1
> Ethernet link redundancy commands
>   redundant-port 1
>   redundant-port force-failover 1
> Ethernet link-fault management
>   outage time of forwarding controller
>     and unified ISSU 1
>   stateful SRP switchover
>     effect on OAM settings 1
>     of more than 2 seconds 1
>     recommendation for PDU loss threshold setting 1
>   stateful SRP switchover support and
>     dependence on completion time 1
>   unified ISSU
>     halted when upgrade in progress 1
>     resumption when upgrade is complete 1
> Ethernet OAM link-fault management
>   actions on exceeding high threshold
>     disabling interface 1
>     failing over to redundant link 1
>   configuring remote failure detection
>     critical events 1
>     dying gasp 1
>     link fault 1
>   configuring, procedure 1
>   disabling
>     remote loopback functionality on a remote peer 1
>   discovery, overview 1
>   elements, overview
>     client 1
>     sublayer 1
>   enabling
>     on a particular interface 1
>     remote loopback functionality on a remote peer 1
>   error message
>     while enabling remote loopback functionality on a remote peer 1
>   example
>     for configuring discovery mode 1
>     for configuring link monitoring 1
>     for configuring remote fault detection 1
>     for enabling remote loopback on local entity 1
>   features, understanding 1
>   figure showing interconnection with LAG 1
>   guidelines for configuring 1
>   implementing
>     at the interface level 1
>   Information OAM PDUs
>     components of 1
>     initiation of discovery in active mode 1
>     transmission settings for 1
>   interrelationship with link aggregation sublayer 1
>   Marker response PDUs
>     and exceeding of high threshold 1
>   modifying
>     discovery mode 1
>   OAM client, functions of 1
>   OAM link monitoring, overview 1
>   OAM messages, overview 1
>   OAM remote and local loopback mode 1
>   OAM remote fault detection, overview 1
>   overview 1
>   performance impact
>     on ES2 4G LMs 1
>   performance impact and memory usage
>     with link monitoring enabled 1
>   platform considerations 1
>   platforms supported for
>     E120 and E320 routers 1
>     ERX7xx, ERX14xx, and ERX310 models 1
>   prerequisite
>     for configuring settings 1
>   references for 1
>   remote loopback start and stop settings
>     not stored across reboots 1
>   setting
>     the local entity into loopback mode 1
>   slow protocols
>     destination address of OAM PDUs and 1
>   specifying
>     action on exceeding high threshold, disabling interface 1
>     action on exceeding high threshold, failover 1
>     detection of remote failure conditions 1
>     high threshold for frame error events 1
>     high threshold for frame seconds summary error events 1
>     high threshold for symbol error events 1
>     interface type 1
>     link events to monitor 1
>     low threshold for frame error events 1
>     low threshold for frame seconds summary error events 1
>     low threshold for symbol error events 1
>     mode of discovery 1
>     PDU loss threshold before link-fault event is generated 1
>     rate of transmission of Information OAM PDUs 1
>     remote loopback functionality 1
>     tracking of error frame events 1
>     tracking of error frame second events 1
>     tracking of symbol error events 1
>     window for frame error events 1
>     window for frame seconds summary error events 1
>     window for symbol error events 1
>   support for unified ISSU 1
>   support on SRP Ethernet interfaces 1
>   supported standards 1
>   viewing
>     configurations for all interfaces on which OAM is enabled 1
>     details about processing of packets, statistics 1
>     discovery mode 1
>     general OAM parameters configured on an interface 1
>     link monitoring configured on an interface 1
>   warning message
>     while placing local entity in remote loopback mode 1
> Ethernet OAM link-fault management commands
>   ethernet oam lfm 1
>   ethernet oam lfm high-threshold 1
>   ethernet oam lfm link-monitor frame-seconds 1
>   ethernet oam lfm link-monitor frame-seconds-summary 1
>   ethernet oam lfm link-monitor symbol-period 1
>   ethernet oam lfm mode 1
>   ethernet oam lfm pdu-lost-threshold 1
>   ethernet oam lfm pdu-transmit-interval 1
>   ethernet oam lfm remote-failure 1
>   ethernet oam lfm remote-loopback start 1
>   ethernet oam lfm remote-loopback stop 1
>   ethernet oam lfm remote-loopback supported 1
>   show ethernet oam lfm discovery 1
>   show ethernet oam lfm statistics 1
>   show ethernet oam lfm status 1
>   show ethernet oam lfm summary 1
> Ethernet OAM messages See OAM messages
> Ethertype value, assigning to S-VLANs 1, 2, 3, 4, 5, 6
> Event notification OAM PDUs
>   description of 1
>   generating to the remote peer 1
>   generation of and sending to the remote peer
>     when low threshold is exceeded 1
>   identification of duplicate events
>     using sequence number 1
>   link monitoring function and 1
>   receive link path monitoring
>     and transmission to the remote peer 1
>   responding to received notices 1
>   supported TLVs for tracking link faults
>     Errored Frame Event 1
>     Errored Frame Seconds Summary Event 1
>     Errored Symbol Period Event 1
>   transmission of, multiple times
>     owing to failure in delivery 1
>   viewing 1
> example 1, 2
> examples, configuration
>   ATM 1483 subinterfaces, dynamic 1
>   ATM VC classes 1, 2
>   bridged Ethernet, dynamic 1
>   bridged Ethernet, static 1
>   Cisco HDLC 1
>   IPoA, dynamic 1
>   MLFR 1
>   MLPPP, dynamic 1
>   MLPPP, static 1, 2
>   Multiclass MLPPP, dynamic 1
>   Multiclass MLPPP, static 1
>   PPPoE, dynamic 1, 2
>   PPPoE, static 1, 2
>   profiles for dynamic interfaces 1
>   transparent bridging 1
>   VLAN subinterfaces, dynamic 1, 2
> exporting ATM 1483 subinterface descriptions 1
> Extensible Authentication Protocol. See EAP
> external loopback 1

F

> F4 OAM cells, for ATM 1
>   configuring 1
>   handling of received cells 1
> F5 OAM cells, for ATM
>   configuring 1, 2
>   disabling automatically 1, 2, 3, 4, 5
>   handling of received cells 1
> failover
>   action on exceeding high threshold
>     OAM link monitoring and 1
>   to secondary link of redundant port
>     on GE-2 and GE-HDE LMs 1
>     when high threshold is exceeded 1
> Fast Ethernet interfaces
>   specifying an interface 1
> Fast Ethernet modules
>   configuring PPPoE 1
>   specifying an interface 1, 2, 3, 4
> fault management, ATM 1
> Flags field
>   in Information OAM PDUs
>     for OAM remote failure detection 1
>   OAM remote fault detection
>     Critical Event bit set in 1
>     Dying Gasp bit set in 1
>     Link Fault bit set in 1
>   viewing
>     configured settings on an interface 1
> flush, ATM OAM 1
> fragmentation
>   Frame Relay packets 1
>   MLPPP
>     configuring dynamic 1
>     configuring static 1
>     overview 1
>   Multiclass MLPPP 1, 2
> frame errors
>   cumulative count of
>     threshold exceptions 1
>   display of aggregated
>     in link event TLVs 1
>     in the show command output 1
>   types of
>     tracked with OAM link monitoring 1
> Frame Relay
>   configuring 1
>   disabling interface 1
>   end-to-end fragmentation and reassembly 1
>     configuring 1
>   error frames 1
>   framing 1
>   interconnection and relationship of NNIs and subnetworks 1
>   map class 1
>   maximum payload size 1
>   monitoring 1
>   multicast addressing 1
>   Network-to-Network Interface 1
>   overview 1
>   platform considerations 1
>   SNMP link status processing 1
>   unicast addressing 1
>   User-to-Network Interface 1
> frame-relay commands 1, See also show frame-relay commands
>   frame-relay class 1
>   frame-relay description 1
>   frame-relay fragment 1
>   frame-relay interface-dlci ietf 1, 2
>   frame-relay intf-type 1
>   frame-relay keepalive 1
>   frame-relay lmi-n391dte 1
>   frame-relay lmi-n392dce 1
>   frame-relay lmi-n392dte 1
>   frame-relay lmi-n393dce 1
>   frame-relay lmi-n393dte 1
>   frame-relay lmi-t391dte 1
>   frame-relay lmi-t392dce 1
>   frame-relay lmi-type 1
>   map-class frame-relay 1
> framing
>   ATM interfaces 1
>   capabilities of E Series routers 1, 2, 3
>   POS interfaces 1

G

> GE-2 line modules
>   with GE-2 SFP I/O modules
>     action when high threshold is exceeded 1
>     action when link fault occurs 1
>     failing over to the redundant link 1
>     failover for remote faults 1
> GE-HDE line modules
>   with GE-2 SFP I/O modules
>     action when high threshold is exceeded 1
>     action when link fault occurs 1
>     failing over to the redundant link 1
>     failover for remote faults 1
> Gigabit Ethernet interfaces for E120 and E320 routers 1, 2, 3
> Gigabit Ethernet modules
>   configuring MLPPP 1
>   configuring PPPoE 1
>   specifying an interface 1, 2, 3, 4, 5, 6
> grace period, dynamic encapsulation type lockout 1
> group (multicast) addressing 1
> groups, bridge. See bridge groups

H

> hash-based packet distribution with MLPPP 1
> HDLC (High-Level Data Link Control), Cisco. See Cisco HDLC
> HDLC (High-Speed Data Link Control)
>   PPP framing 1
>   serial encapsulation 1
> hdlc commands
>   hdlc down-when-looped 1
>   hdlc keepalive 1
>   hdlc shutdown 1
> high availability
>   and atm atm1483 subscriber command 1
>   and subscriber command 1, 2, 3
> high threshold
>   action when exceeded on
>     GE-2 LMs with GE-2 SFP I/O modules 1
>     GE-HDE LMs with GE-2 SFP I/O modules 1
>   actions performed on exceeding
>     failing over to the redundant link 1
>     moving the interface state to down, disabling 1
>   for OAM link monitoring
>     action taken when exceeded 1
>     when exceeded, disabling the interface 1
>     when exceeded, failover to secondary link 1
>   specifying
>     for frame error events 1
>     for frame seconds summary error events 1
>     for symbol error events 1
>   when exceeded
>     default action taken 1
> high threshold setting
>   configuring for an interface
>     for link monitoring 1
> high threshold value
>   recommendation on setting
>     for link-fault monitoring 1
> High-Level Data Link Control. See Cisco HDLC
> High-Speed Data Link Control. See HDLC
> higher-level protocols over Ethernet
>   platform considerations 1

I

> IEEE 802.1Q 1
> IEEE 802.1w 1
> IEEE 802.1w (Rapid Reconfiguration of Spanning Tree) 1
> IEEE 802.3ad 1
> IEEE 802.3ad (Link Aggregation) 1
> IEEE 802.3ah OAM link-fault management See Ethernet OAM link-fault management
> ILMI 1
> ILMI (integrated local management interface)
>   about 1
>   enabling 1
>   keepalive timer 1
> inarp command 1, 2
> individual (unicast) addressing 1
> Information OAM PDUs
>   bandwidth allocation for OAM traffic
>     using the OAM sublayer capabilities TLV 1
>   bidirectional transmission of
>     keepalive for OAM association 1
>   components, overview 1
>   contained TLV fields
>     OAM sublayer capabilities 1
>     state 1
>     vendor OUI 1
>     vendor-specific details 1
>   description of 1
>   forwarding to the remote peer in cases
>     where no other types of OAM PDUs are ready for sending 1
>   loss threshold setting
>     action taken when configured value is exceeded 1
>     definition of 1
>   maximum transmission rate
>     impact on performance 1
>   receipt by the remote peer
>     and wait time for obtaining local entity details 1
>     determination of formation of OAM association 1
>   reestablishment of OAM association
>     link-fault event clearance 1
>   restart of discovery
>     link-fault event generation 1
>   scenario of OAM association failure
>     with remote peer not supporting loopback 1
>   timer setting
>     maximum value 1
>     minimum value 1
>     rate of transmission in milliseconds 1
>   transmission settings for, overview 1
>   transmission to the remote entity
>     triggering of the discovery process and 1
>   using the Flags field of
>     and OAM remote fault detection 1
>   viewing 1
>   with Link Fault event bit set
>     not containing TLV data 1
> integrated local management interface. See ILMI
> interface commands
>   interface atm 1, 2, 3, 4, 5, 6, 7, 8, 9
>   interface fastEthernet 1, 2, 3, 4, 5, 6
>   interface gigabitEthernet 1, 2, 3, 4, 5, 6
>   interface lag 1
>   interface mlframe-relay 1
>   interface mlppp 1, 2
>   interface pos 1, 2, 3, 4
>   interface serial 1
>     Cisco HDLC interfaces 1
>     Frame Relay interfaces 1, 2
>     PPPoE interfaces 1
>   interface tenGigabitEthernet 1, 2, 3, 4, 5, 6
> interface description
>   Frame Relay interfaces 1
>   POS interfaces 1, 2
>   serial interfaces 1
> interfaces
>   10-Gigabit Ethernet 1, 2, 3, 4, 5, 6
>   bridge. See bridge interfaces
>   Fast Ethernet 1, 2, 3, 4
>   Gigabit Ethernet 1, 2, 3, 4, 5, 6
>   serial. See serial interfaces
> interfaces, monitoring
>   Ethernet 1, 2, 3
> internal loopback 1
> International Telecommunication Union. See ITU
> Internet Protocol Control Protocol. See IPCP
> interworking function See IWF
> Inverse ARP 1
> IP addresses
>   assigning to Cisco HDLC interfaces 1
>   assigning to Frame Relay subinterfaces 1, 2
>   assigning to PPP interface 1
>   PPPoE interfaces 1, 2, 3
> ip commands
>   ip (subscriber policies) 1
>   ip access-routes 1
>   ip address 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11
>   ip auto-configure ip-subscriber 1
>   ip auto-detect ip-subscriber 1
>   ip directed-broadcast 1
>   ip filter-options all 1
>   ip igmp 1
>   ip ignore-df-bit 1
>   ip inactivity-timer 1
>   ip mac-validate 1
>   ip mtu 1
>   ip nat 1
>   ip policy 1
>   ip redirects 1
>   ip route-map ip-subscriber 1
>   ip sa-validate 1
>   ip tcp adjust-mss 1
>   ip unnumbered 1, 2
>   ip virtual-router 1
> IP over ATM. See IPoA
> IP over VLAN over bridged Ethernet 1
> IP profile 1
> IP routes, inserting dynamic routes intorouting table 1
> IPCP (Internet Protocol Control Protocol)
>   option 0x90 1
>   overview 1
> IPoA (IP over ATM)
>   configuring dynamic interfaces 1
>   dynamic interfaces 1, 2
> IPv4 and IPv6 over Static PPPoE
>   IPv4 and IPv6 interface columns 1
> IPv6
>   neighbor discovery, defining 1
> ipv6 commands
>   ipv6 address 1
>   ipv6 mld 1
>   ipv6 mtu 1
>   ipv6 nd 1
>   ipv6 nd managed-config-flag 1
>   ipv6 nd other-config-flag 1
>   ipv6 nd prefix-advertisement 1
>   ipv6 nd ra-interval 1, 2
>   ipv6 nd reachable-time 1
>   ipv6 nd suppress-ra 1
>   ipv6 policy 1
>   ipv6 sa-validate 1
>   ipv6 unnumbered 1
>   ipv6 virtual-router 1
> IPv6 neighbor discovery commands
>   ipv6 nd reachable-time 1
> IPv6 profile 1
> ITU (International Telecommunication Union) recommendation, ATM OAM standards 1
> IWF
>   configuration scenarios
>     multiple DSLAMs connected to an access concentrator 1
>     single DSLAM connected to an access concentrator 1
>   defined by the DSL Forum
>     for conversion of PPPoA and PPPoE over ATM sessions 1
>   definition of, uses 1
>   enabling migration of DSL networks
>     from ATM to Ethernet links 1
>   PPPoE sessions
>     dynamic encapsulation type lockout 1
>     with duplicate MAC addresses 1, 2, 3
>     with duplicate protection feature enabled 1
> IWF PPPoE sessions
>   duplicate protection of
>     guidelines for configuring 1
>   dynamic encapsulation type lockout
>     configuration example 1
>     guidelines for configuring 1
>     using DSL Forum VSAs as criteria 1
>   processing of
>     duplicate MAC addresses in multiple sessions 1
>     dynamic encapsulation type lockout 1
>   with duplicate MAC addresses of clients
>     ATM-to-Ethernet interworking 1
>     dependence on pppoe sessions command configuration 1
>     limit on maximum number of sessions 1
>     scenario, multiple DSLAMs linked to a B-RAS 1
>     scenario, single DSLAM linked to a B-RAS 1
> IWF PPPoE tag
>   insertion in the PADR packet
>     sent from the PPPoE client to the access concentrator 1
>   used to distinguish
>     between an IWF and a non-IWF PPPoE session 1
> IWF-Session DSL Forum VSA
>   absence in PADR packets
>     duplicate protection, disabled 1
>     duplicate protection, enabled 1
>   presence in PADR packets
>     and B-RAS application 1, 2
>     duplicate protection, disabled 1
>     duplicate protection, enabled 1
>     duplicate protection, guidelines 1
>     dynamic encapsulation type lockout 1
>     enabling multiple sessions with the same MAC address 1
>   suboption for
>     field code 1
>     length field, value 1

J

> J-Flow commands
>   ip route-cache flow sampled 1

K

> keepalive timer, setting 1

L

> L2TP (Layer 2 Tunneling Protocol) 1
>   profile characteristics 1
>   using PPPoE remote circuit ID 1, 2
> l2tp commands
>   l2tp policy 1
> L2TP Proxy Authenticate Extensions for EAP—draft-ietf-l2tpext-proxy-authen-ext-eap-01.txt (December 2006 expiration) 1
> LACP (Link Aggregation Control Protocol) 1
>   PPPoE subinterfaces 1, 2
>   redundant member link behavior 1
> LAG bundle
>   position of
>     and OAM link-fault management 1
>     between OAM sublayer and MAC client 1
> LAG member link
>   marked as redundant
>     using link monitoring for failover and link reversal 1
> LAG multiplexer
>   feeding LAC protocol logic 1
>   feeding link events 1
> layer 2 services over MPLS
>   802.3ad link aggregation 1
>   802.3ad switch 1
> Layer 2 Tunneling Protocol. See L2TP
> LCP (Link Control Protocol)
>   configuration options 1, 2, 3
>     endpoint discriminator 1
>     MRRU 1
>     Multilink header format 1
>     Prefix elision 1
>     SSN header format 1
>   restarting negotiations for PPPoA clients 1
> Link Control Protocol. See LCP
> link events
>   and processing of LAC protocol logic 1
>   local generation of
>     using health monitoring 1
>   supplied to the LAG multiplexer 1
> link fault
>   bit set in the Flags field
>     influencing the link state based on 1
>   example condition of occurrence 1
>   loss of signal detection
>     by the receiver 1
>   rate of transmission
>     in Information OAM PDUs 1
> Link fault information OAM PDUs
>   detection of receive path failure 1
>   sending of
>     not supported 1
> Link Integrity Protocol. See LIP
> link monitoring
>   frequent polling of error counters
>     when enabled on the local entity 1
>   impact on performance and memory usage
>     when disabled on the local entity 1
>     when enabled on the local entity 1
> link monitoring, of Ethernet interfaces See OAM link monitoring
> link-fault event
>   clearing of
>     interface transition to the up state 1
>     reestablishment of OAM association 1
>   generation of
>     non-receipt of OAM PDUs within the loss threshold 1
> link-fault management commands
>   for Ethernet interfaces
>     show ethernet oam 1
> link-fault management, Ethernet interfaces See Ethernet OAM link-fault management
> LIP (Link Integrity Protocol) 1
> LMI (local management interface)
>   configuring counters and timers 1
>   configuring type 1
>   enabling 1
>   monitoring 1, 2, 3
> load-interval command
>   ATM interfaces 1
>   POS interfaces 1
> local loopback mode See OAM loopback mode
> local management interface. See LMI;ILMI
> local OAM entity
>   health monitoring threshold exceeded
>     failover to secondary link 1
>   prerequisite for configuring
>     remote loopback on 1
>   preventing both local and remote entities
>     from simultaneous loopback 1
>   retrieval and response to performance variables
>     in active mode 1
>   sending of performance variables to peer
>     support for 1
>   transmission of Information OAM PDUs
>     receipt by the remote peer 1
> lockout, encapsulation type. See dynamic encapsulation type lockout
> log severity debug command 1, 2
> loopback
>   detection on Cisco HDLC interfaces 1
> loopback command
>   ATM interfaces 1
>   POS interfaces 1
> Loopback control OAM PDUs
>   description of 1
>   sending of
>     for termination of loopback 1
>   start of loopback of remote peee
>     by local entity 1
>   viewing 1
> loopback for ATM VC integrity
>   cells 1
>   configuring 1, 2
>   F4 OAM cells 1
>   handling of received cells 1
> loopback frames
>   forwarding of
>     from the parser to the subordinate sublayer 1
>   processing by the packet parser
>     transmission to the multiplexer 1
> lost-link timer
>   and Ethernet OAM link-fault management 1
>   equivalent to
>     product of PDU timer and loss threshold 1
>   resetting OAM discovery 1
> low threshold
>   for OAM link monitoring
>     generation of Event notification PDU 1
>     response when exceeded 1
>   specifying
>     for frame error events 1
>     for frame seconds summary error events 1
>     for symbol error events 1
> low threshold value
>   recommendation for setting
>     for link-fault monitoring 1

M

> MAC (media access control) addresses
>   bridging overview 1
>   configuring for S-VLANs 1, 2
>   configuring for VLANs 1
>   removing from forwarding table 1
>   using with bridged Ethernet 1
>   validation on bridged Ethernet interfaces 1
> MAC address
>   usage in dynamic encapsulation lockout
>     for IWF PPPoE sessions 1
> macro command 1
> macros
>   using to configure dynamic interfaces 1
> magic numbers 1
> manuals
>   comments on 1
> map class, Frame Relay fragmentation 1
> map entries, Frame Relay 1, 2
> map list, using to configure NBMA interfaces 1
> map-class frame-relay command 1
> map-group command 1
> map-list command 1
> Marker response OAM PDUs
>   circumstances of non-transmission of 1
>   link event caused by exceeding high threshold
>     and disabling sending of 1
> maximum payload size, Frame Relayfragmentation 1
> maximum receive unit. See MRU
> media access control addresses See MAC addresses
> member-interface command 1, 2, 3
> message of the minute messages. See MOTM messages
> MFR
>   aggregating OC3/STM1 lines 1
> MLFR (Multilink Frame Relay)
>   aggregating T1 or E1 lines 1
>   aggregation limits 1
>   bundle 1, 2
>   bundle limits 1
>   configuring 1
>   interfaces, monitoring 1
>   Link Integrity Protocol 1
>   member link sequence numbers 1
>   NxT1 service 1
>   overview 1
>   packet distribution, round-robin 1
>   platform considerations 1
>   protocol layering 1
>   unsupported features 1
> MLP. See MLPPP
> MLPPP (Multilink PPP) 1, See also ppp commands
>   aggregating T1 or E1 lines 1
>   aggregation limits 1
>   authentication 1
>   bundle 1, 2
>   bundle limits 1
>   bundle name and RADIUS 1
>   commands, contextual differences of 1
>   configuring 1
>   ECMP 1
>   encapsulation 1
>   endpoint discriminator 1
>   features 1
>   fragmentation
>     configuring dynamic 1
>     configuring static 1
>     overview 1
>   interface stacking 1
>   interfaces, monitoring 1
>   member link sequence numbers 1
>   MRRU 1
>   NxT1 service 1
>   overview 1
>   packet distribution 1
>   platform considerations 1
>   profiles 1
>   protocol layering 1
>   reassembly
>     configuring dynamic 1
>     configuring static 1
>     overview 1
>   SSN header format 1
>   statistics and baselining 1
>   unsupported features 1
> modules
>   ATM capabilities 1
> monitor commands
>   monitor atm vc 1
>   monitor atm vp 1
>   monitor vlan interface 1
> monitoring. See specific feature, product, or protocol
> MOTM (message of the minute) messages 1
> MP. See MLPPP
> MPLS (Multiprotocol Label Switching)
>   configuring over Ethernet link aggregation 1
>   configuring S-VLAN tunnels 1, 2
> mpls commands
>   mpls 1, 2
>   mpls (subscriber policies) 1
>   mpls atm vci range 1
>   mpls-relay 1
> MPLS over VLAN over bridged Ethernet 1
> MRRU LCP configuration option 1
> MRU (maximum receive unit)
>   POS interfaces 1
>   PPP interfaces 1, 2
> mru command 1
> MTU (maximum transmission unit) See MTU
>   bridged Ethernet interfaces 1
>   Ethernet interfaces 1
>   POS interfaces 1
> mtu command 1
>   Ethernet interfaces 1, 2
> multicast addressing 1
> multicast command 1
> Multiclass MLPPP
>   configuration guidelines 1
>   configuring 1
>   enabling 1
>   example, dynamic 1
>   example, static 1
>   fragmentation 1, 2, 3
>   monitoring 1
>   overview 1
>   platform considerations 1
>   reassembly 1, 2, 3
>   traffic-class 1, 2, 3, 4
> Multilink Frame Relay. See MLFR
> multilink maximum received reconstructed unit (MRRU) 1
> Multilink PPP. See MLPPP
> multinetting 1
> multiplexer
>   pass-through of MAC client-generated frames
>     without any modification 1
>   transfer of loopback frames
>     forwarded to the subordinate sublayer 1
>     received from the parser 1
>   working of
>     for link-fault management of Ethernet interfaces 1
> multipoint, ATM connections 1, 2

N

> NBMA 1
> NBMA (nonbroadcast multiaccess) 1
>   configuring 1
>   description 1
>   Inverse ARP 1
>   point-to-multipoint 1
>   removing circuits 1
>   static mapping 1
> nested profile assignments
>   VLAN subinterfaces 1
> NNI (Network-to-Network Interface),Frame Relay 1, 2, 3
> nonbroadcast multiaccess. See NBMA
> notice icons 1
> NxT1 service
>   MLFR 1
>   MLPPP 1

O

> OAM (Operation, Administration, and Management), ATM 1
>   cc (continuity check) cells 1
>   configuring 1, 2
>   disabling F5 OAM services 1, 2, 3, 4, 5
>   flush 1
>   standards 1
> OAM association
>   after establishment of
>     transmission rate and packet loss threshold settings 1
>   formation of 1
>   keepalive for
>     using bidirectional transfer of OAM PDUs 1
>   rebuilding of
>     operational up state of the interface and 1
>   successful rediscovery with the remote peer
>     link transition to the up state 1
>   tearing down of
>     generation of the link-fault event 1
> OAM client
>   enabling and configuration of OAM sublayer 1
>   enabling OAM operations on the link
>     during the discovery phase 1
>   management of
>     remote loopback functionality 1
>     responses to OAM PDUs received from the remote peer 1
>   monitoring OAM PDUs from the remote peer 1
> oam commands
>   oam ais-rdi 1, 2
>   oam cc 1, 2
>   oam retry 1, 2
>   oam-pvc 1, 2
> OAM discovery
>   automatic activation of 1
>   configuration at the interface level 1
>   controlling other OAM attributes for an entity 1
>   enabling on an interface 1
>   exceeding of PDU loss threshold
>     link transition to the down state 1
>   first phase of OAM association 1
>   implementation of
>     by the control block 1
>   interconnection with
>     loopback operation 1
>     variable requests 1
>   monitoring the remote peer 1
>   restarting of
>     Information OAM PDU loss threshold 1
>   restriction on performing
>     scenario in which it occurs 1
>   successful rediscovery with the remote peer
>     link transition to the up state 1
>   supported types
>     active mode 1
>     passive mode 1
>   topology for configuration of
>     customer edge devices 1
>     provider edge devices 1
> OAM discovery mode
>   configuring 1
>   example, configuring 1
>   monitoring 1
> OAM elements
>   operations of
>     and link-fault management 1
>   parts of
>     client 1
>     sublayer 1
> OAM features
>   backward compatibility with older networks 1
>   benefits of 1
>   IEEE 802.3ah enhancements and 1
>   supported 1
>   types of
>     discovery 1
>     link monitoring 1
>     remote and local loopback 1
>     remote fault detection 1
> OAM link monitoring
>   actions on high threshold excess
>     disabling interface 1
>     failing over to the redundant link 1
>   advertisement of OAM attributes
>     using Information OAM PDUs 1
>   continuation with a new window
>     when the link is in up state 1
>   detecting frame and symbol errors 1
>   error frame seconds summary
>     overview of 1
>   error frames per second
>     overview of 1
>   error symbols per second
>     overview of 1
>   example, configuring 1
>   generation of Event notification OAM PDUs
>     when low threshold is exceeded 1
>   health and quality analysis of the link
>     using tracking of frame and symbol errors 1
>   improving failover and recovery times
>     configuration of OAM sublayer 1
>   influencing the link state
>     on exceeding link quality threshold 1
>     on receipt of a critical event PDU from peer 1
>   influencing the operational link state
>     when high threshold is exceeded 1
>   overview of feature 1
>   period for detecting errors 1
>   physical redundancy
>     preservation of MAC bindings 1
>     preservation of the same MAC address 1
>     switchover from primary to secondary link 1
>     without indicating to higher-layer protocols 1
>   repeated sending of Event notification PDUs
>     preventing duplication 1
>   supported error events
>     error frame 1
>     error frame seconds summary 1
>     error symbol period 1
>   supported frame errrors tracked
>     alignmentError 1
>     frameCheckSequence 1
>     frameTooLong 1
>     lengthError (runts) 1
>   symbol errors counting
>     on IOAs that do not support 1
>   threshold for frame, symbol errors 1
>   using Event notification OAM PDUs 1
>   using the results of
>     to configure LAG sublayer 1
>   viewing configured values 1
> OAM link-fault event See link-fault event
> OAM link-fault management See Ethernet OAM link-fault management
> OAM link-fault management, 802.3ah 1
> OAM loopback mode
>   cessation by the initiating entity
>     using Loopback control PDUs 1
>   configuring 1
>   higher priority for OAM PDUs
>     over data traffic 1
>   in disabled state
>     receipt of Information PDUs by local entity 1
>     restarting sending of locally sourced non-OAM PDUs 1
>   in enabled state
>     received data calculation 1
>     transmitted data calculation 1
>   initiation phase
>     discarding locally sourced non-OAM PDUs 1
>   intentional discard of data frames
>     by remote peer 1
>   local and remote functionalities
>     overview 1
>   preventing loopback on both local and remote entities
>     verification to perform 1
>   processing of OAM PDUs
>     measuring link performance 1
>   remote
>     feature supported by the remote peer 1
>     link quality between local and remote entities 1
>     non-OAM PDUs resent to the local entity 1
>     placing a peer into loopback mode 1
>     processing of OAM PDUs 1
>   settings for enabling and disabling remote loopback
>     not stored across reboots 1
>   viewing configuration 1
>   warning message
>     while placing local entity in remote loopback 1
> OAM messages
>   format of
>     Code field, usage 1
>     Data/Pad field, usage 1
>     Flags field, usage 1
>   format of, figure 1
>   forwarding to the control block 1
>   higher priority over data traffic
>     during remote loopback 1
>   length of untagged frames 1
>   maximum transmission rate
>     performance impact 1
>   processing by multiplexer 1
>   processing by the packet parser 1
>   processing during remote loopback
>     measuring link performance 1
>   properties of
>     determination of maximum frame size 1
>     rate of transmission per second 1
>     size range 1
>     value of destination MAC address 1
>     value of Ethertype 1
>     value of frame payload 1
>   rules management of received
>     by the control block 1
>   supported types
>     Event notification OAM PDUs 1
>     Information OAM PDUs 1
>     Loopback control OAM PDUs 1
>     Vendor-specific OAM PDUs 1
>   transmission of
>     control block and 1
>   transmission rate and
>     impact on router operations 1
>   with link-fault event bit in Flags field
>     higher preferential processing 1
> OAM PDU loss threshold
>   actions taken when exceeded
>     link problem signalled 1
>     link transition to the down state 1
>   configuring 1
>   definition of
>     action taken when configured value is exceeded 1
>   product of transmission rate and
>     equals lost-link timer 1
>   recommendation for setting
>     for link-fault monitoring 1
>   viewing configured value 1
> OAM PDU transmission rate
>   configuring 1
>   definition of
>     range for configuration 1
>   product of loss threshold and
>     equals lost-link timer 1
>   viewing configured setting 1
> OAM PDUs See OAM messages
> OAM remote failure monitoring See OAM remote fault detection
> OAM remote fault detection
>   action when link fault occurs
>     disabling interface 1
>     failing over to secondary port 1
>   conditions notified using
>     Flags field of Information OAM PDU 1
>   example, configuring 1
>   monitoring the receive link path
>     generation of Event notification PDUs 1
>   types of failures monitored
>     critical event 1
>     dying gasp 1
>     link fault 1
> OAM remote loopback settings
>   viewing 1
> OAM session
>   changed to down, nonfunctional
>     after the action for high threshold excess is taken 1
>   in down state with loss of OAM association
>     status in show command output 1
> OAM state machine
>   port in the down state
>     until discovery process completion 1
> OAM sublayer
>   below the 802.3ad LAG sublayer
>     interworking with link aggregation 1
>   capabilities of
>     assessment of supported functions for remote entities 1
>     bandwidth utilization for OAM traffic 1
>     maximum OAM PDU size for sending and receiving 1
>     rate limit on number of frames transferred 1
>   components of
>     control block, functions 1
>     multiplexer, functions 1
>     packet parser, functions 1
>   interworking with link aggregation
>     situated below the LAG bundle 1
>   placement of
>     above the MAC layer 1
>     below the LLC layer 1
>   presentation of interface to clients
>     for MAC clients 1
>     for OAM clients 1
> OAM traffic
>   higher priority over data frames
>     when oversubscription occurs 1
> OC3 modules
>   monitoring ATM interfaces 1
>   testing ATM interfaces 1
> OCx/STMx interfaces
>   MLPPP features 1
> Operation, Administration, and Maintenance, Ethernet interfaces See Ethernet OAM link-fault management
> Operation, Administration, and Management. See OAM, ATM
> option 82 field, DHCP 1
> OSI Network Layer Control Protocol. See OSINLCP
> OSINLCP (OSI Network Layer Control Protocol) 1
> overriding base profile assignments
>   assigning to PVC 1
>   monitoring 1, 2
>   overview 1, 2
>   removing from PVC 1
>   removing from VC range or subrange 1
>   removing from VLAN range or subrange 1
>   removing from VLAN subinterface 1
>   VLANs 1
> oversubscription
>   dynamic ATM interfaces 1, 2
>   S-VLANs 1
> oversubscription of allotted bandwidth
>   discarding of data traffic
>     higher priority for OAM PDUs 1
>     with peer in loopback 1

P

> packet logging, PPP and PPPoE 1
> packet over SONET. See POS
> packet parser
>   classification of received frames
>     and forwarding to appropriate entities 1
>   delivery of OAM PDUs
>     to the control block 1
>   working of
>     for OAM link-fault management 1
> PADM (PPPoE Active Discovery Message), configuring 1
> PADN (PPPoE Active Discovery Network) messages, configuring 1
> padn command 1
> PADR (PPPoE Active Discovery Request)
>   IWF PPPoE sessions
>     criteria for encapsulation type lockout 1
>   IWF-Session DSL VSA absent in
>     duplicate protection disabled 1
>     duplicate protection enabled 1
>   IWF-Session DSL VSA present in
>     duplicate protection disabled 1
>     duplicate protection enabled 1
>     suboptions, field code 1
>     suboptions, length field 1
>   with IWF-Session DSL VSA
>     for differentiating between IWF and non-IWF sessions 1
>     from access nodes to the DSLAM 1
> PADS (PPPoE Active Discovery Session) packets, configuring 1
> PAP (Password Authentication Protocol) 1
> passive discovery mode
>   and OAM link-fault management 1
>   configuration on
>     customer edge devices 1
>   enabled on local and remote entities
>     and influence on discovery process 1
>   working of 1
> Password Authentication Protocol. See PAP
> payload, ATM cell 1
> PCR (peak cell rate) 1
> PDU loss threshold See OAM PDU loss threshold
> performance impact
>   with link-fault management
>     frequency of querying MAC-layer statistics 1
>     frequency of retrieval of errored symbols 1
>     maximum frequency of PDUs transmission 1
>     on ES2 4G LMs 1
> performance variables
>   for link-fault management
>     retrieval and response to 1
>     sending of 1
> permanent virtual circuit. See PVC
> physical level redundancy
>   OAM link monitoring
>     preservation of MAC bindings 1
>     preservation of the same MAC address 1
>     switchover from primary to secondary link 1
>     without indicating to higher-layer protocols 1
> physical link redundancy
>   on GE-2 and GE-HDE line modules
>     action performed on exceeding high threshold 1
>     failing over to redundant link 1
> ping atm interface atm command 1
> ping, ATM
>   configuring 1
>   overview 1
> platform considerations
>   ATM 1
>   bridged Ethernet 1
>   bridged IP 1
>   Cisco HDLC 1
>   dynamic interfaces 1, 2, 3
>   Ethernet interfaces 1
>   Frame Relay 1
>   higher-level protocols over Ethernet 1
>   MLFR 1
>   MLPPP 1
>   Multiclass MLPPP 1
>   OAM link-fault management 1
>   POS 1
>   PPP 1
>   PPPoE 1
>   transparent bridging 1
> point-to-multipoint, NBMA connection 1
> Point-to-Point Protocol over ATM. See PPPoA
> Point-to-Point Protocol over Ethernet. See PPPoE
> Point-to-Point Protocol. See PPP
> policies, subscriber. See subscriber policies for transparent bridging
> policy commands
>   atm policy 1, 2
>   frame-relay policy 1, 2
>   gre-tunnel policy 1, 2
>   ip policy 1
>   l2tp policy 1, 2
>   mpls policy 1, 2
>   vlan policy 1, 2
> policy management
>   baselining statistics 1
>   preserving statistics 1
>   statistics 1
> POS (packet over SONET)
>   configuring interface 1
>   disabling interface 1
>   E120 and E320 routers 1, 2, 3, 4
>   E320 routers 1
>   line modules supported 1
>   monitoring interface 1
>   overview 1
>   platform considerations 1
>   references 1
> pos commands
>   pos description 1, 2, 3
>   pos framing 1
>   pos scramble-atm 1
> PPP (Point-to-Point Protocol)
>   accounting statistics for terminated sessions 1
>   Async-Control-Character-Map (ACCM) option 1
>   authentication 1, 2, 3
>   configuring 1
>   configuring dynamic interfaces 1
>   E120 and E320 routers 1, 2
>   E320 routers 1
>   EAP 1
>   Extensible Authentication Protocol 1
>   interfaces 1
>   magic numbers 1
>   monitoring interfaces 1
>   network control protocol 1
>   packet logging 1
>   platform considerations 1
>   PPP profiles 1
>   troubleshooting
>     dynamic interfaces 1
>     static interfaces 1
> ppp commands 1, See also show ppp commands
>   ppp aaa-profile 1
>   ppp authentication 1, 2, 3
>   ppp chap-challenge-length 1, 2
>   ppp description 1
>   ppp fragmentation 1, 2
>   ppp hash-link-selection (MLPPP) 1, 2
>   ppp initiate-ip 1
>   ppp initiate-ipv6 1
>   ppp ipcp netmask 1
>   ppp keepalive 1, 2
>   ppp keepalive (MLPPP) 1
>   ppp log 1, 2
>   ppp log (MLPPP) 1
>   ppp magic-number disable 1, 2
>   ppp magic-number disable (MLPPP) 1
>   ppp magic-number ignore-mismatch 1, 2, 3
>   ppp max-bad-auth 1
>   ppp max-bad-auth (MLPPP) 1
>   ppp max-negotiations 1, 2, 3
>   ppp mru 1, 2, 3
>   ppp multilink enable (MLPPP) 1, 2, 3
>   ppp passive-mode 1, 2
>   ppp passive-mode (MLPPP) 1
>   ppp peer 1, 2, 3
>   ppp peer (MLPPP) 1
>   ppp reassembly 1, 2
>   ppp shutdown 1
>   ppp shutdown (MLPPP) 1
>   ppp shutdown ip 1
>   ppp shutdown mpls 1
>   ppp shutdown osi 1
> PPP Multilink. See MLPPP
> PPPoA (Point-to-Point Protocol over ATM)
>   terminating stale subscribers and restarting LCP negotiations 1
> PPPoE 1
> PPPoE (Point-to-Point Protocol over Ethernet)
>   Active Discovery Initiation (PADI) packets 1
>   Active Discovery Message (PADM) 1
>   Active Discovery Network (PADN) messages 1
>   Active Discovery Offer (PADO) packets 1
>   Active Discovery Request (PADR) packets 1
>   Active Discovery Session (PADS) packets 1, 2
>   agent-circuit-identifier information 1
>   capturing remote circuit ID
>     configuring 1
>     dsl-forum-1 format and examples 1, 2
>     formatting 1, 2
>     monitoring 1
>     overview 1
>     sending to RADIUS or L2TP 1, 2
>     troubleshooting 1
>     using in profiles 1, 2
>   configuring dynamic interfaces over ATM 1
>   configuring dynamic interfaces over PPPoE 1
>   configuring for Ethernet 1, 2
>   configuring over ATM 1
>   Discovery protocol 1
>   DSL Forum VSA 26-1 1
>   duplicate protection of
>     IWF PPPoE sessions, guidelines for configuring 1
>     IWF PPPoE sessions, processing of 1
>     IWF PPPoE sessions, scenarios 1
>     non-IWF PPPoE sessions, scenarios 1
>   duplicate protection scenarios for IWF PPPoE sessions
>     1:1 association between DSLAMs and the B-RAS 1
>     N:1 association between DSLAMs and the B-RAS 1
>   dynamic encapsulation type lockout 1, 2, See also and IWF PPPoE sessions
>     clearing lockout condition 1
>     configuring 1
>     differences from PPPoE over static ATM 1
>     monitoring 1, 2, 3, 4, 5
>   E120 and E320 routers 1, 2
>   monitoring interfaces 1
>   overview 1
>   packet logging 1
>   platform considerations 1
>   subinterfaces for LACP 1, 2
>   troubleshooting
>     dynamic interfaces 1
>     static interfaces 1
> PPPoE access concentrator
>   connected to a single DSLAM
>     for IWF sessions 1
>   connected to multiple DSLAMs
>     for IWF sessions 1
>   IWF PPPoE sessions
>     duplicate protection of 1
>     dynamic encapsulation type lockout 1
> pppoe commands 1, See also show pppoe commands
>   encapsulation pppoe 1
>   pppoe 1, 2, 3, 4
>   pppoe (subscriber policies) 1
>   pppoe acname 1, 2, 3
>   pppoe always-offer 1
>   pppoe auto-configure 1
>   pppoe auto-configure lockout-time 1
>   pppoe clear lockout interface 1
>   pppoe duplicate-protection 1, 2, 3
>   pppoe log pppoeControlPacket 1
>   pppoe motm 1, 2, 3, 4
>   pppoe pads disable-ac-info 1
>   pppoe profile 1
>   pppoe remote-circuit-id 1, 2
>   pppoe service-name-table 1, 2, 3, 4
>   pppoe sessions 1, 2
>   pppoe subinterface 1, 2, 3
>   pppoe subinterface fastEthernet 1
>   pppoe subinterface gigabitEthernet 1
>   pppoe subinterface lag 1
>   pppoe subinterface tenGigabitEthernet 1
>   pppoe url 1, 2, 3
>   service 1
> PPPoE over S-VLAN over bridged Ethernet 1
> PPPoE over VLAN over bridged Ethernet 1
> PPPoE service name tables
>   action, defined 1
>   configuring 1
>   creating and populating 1
>   enabling for dynamic interfaces 1
>   enabling for static interfaces 1
>   Ethernet configurations 1
>   overview 1
>   service name tag, defined 1
> PPPoE sessions
>   with IWF-Session DSL Forum VSA See IWF PPPoE sessions
>   with IWF-Session DSL VSA
>     contained in PADR packets 1
>     duplicate MAC addresses of the DSLAM 1
>     limit on maximum number of sessions 1
> precedence levels for VC classes
>   examples 1
>   overview 1
> prerequisite
>   for configuring link-fault management
>     on Ethernet interfaces 1
>   for enabling remote peer to loop back PDUs 1
> privilege level
>   for troubleshooting dynamic interfaces 1, 2
> profile commands 1, See also show profile commands
>   profile 1, 2, 3, 4, 5, 6, 7, 8, 9
>   profile atm1483 bulk-config-name 1, 2
>   profile atm1483 bulk-config-name pvc 1
>   profile vlan bulk-config 1
>   profile vlan override 1
>   profile-reassign 1, 2, 3
>   vlan profile 1, 2
>   vlan service-profile 1
> profiles
>   assigning to a static interface 1
>   assigning to an interface 1
>   characteristics for 1
>   creating for debugging 1
>   description 1, 2
>   for dynamic ATM 1483 subinterfaces 1
>   for dynamic VLAN subinterfaces 1
>   monitoring 1, 2
>   overriding base profile assignments 1, 2, 3, 4
>   reassigning for troubleshooting 1
>   using to configure dynamic interfaces 1
>   working with 1
> protocol data units (PDUs)
>   number that the remote peer can fail to receive
>     specifying 1
>   rate of transmission of
>     specifying 1
>   standard length of
>     for link-fault management of Ethernet interfaces 1
> proxy ARP 1
> PVC (permanent virtual circuit)
>   assigning VC classes 1
>   ATM interfaces 1, 2, 3
>   bulk configuration of 1
>   configuring encapsulation 1
>   configuring F5 OAM 1
>   configuring for bridged IP 1
>   configuring individual parameters for 1
>   configuring Inverse ARP 1
>   configuring service category 1
>   creating control PVCs 1
>   creating data PVCs 1
>   Frame Relay 1, 2, 3, 4
>   overview 1
> pvc command
>   for control PVCs 1
>   for data PVCs 1

R

> RADIUS (Remote Authentication Dial-In User Service)
>   authentication of dynamic interfaces 1, 2, 3
>   configuring dynamic interfaces from 1
>   MLPPP Bundle Name VSA 1
>   overriding attributes for PPPoE 1, 2
>   using PPPoE remote circuit ID 1, 2
> radius commands
>   radius override calling-station-idremote-circuit-id 1
>   radius override nas-port-id remote-circuit-id 1
>   radius remote-circuit-id-delimiter 1, 2
>   radius remote-circuit-id-format 1, 2
>   radius remote-circuit-id-format (dsl-forum-1 keyword) 1, 2
> ranges, VC. See VC ranges, bulk configuration of
> ranges, VLAN See VLAN ranges, bulk configuration of RDI (remote defect indication) cells
> RDI (remote defect indication) cells 1, 2
> reassembly
>   Frame Relay packets 1
>   MLPPP
>     configuring dynamic 1
>     configuring static 1
>     overview 1
>   Multiclass MLPPP 1, 2
> reassigning profiles to dynamic interfaces 1
> relearn command 1
> remote circuit ID, capturing for PPPoE
>   configuring 1
>   dsl-forum-1 format and examples 1, 2
>   formatting 1, 2
>   monitoring 1
>   overview 1
>   sending to RADIUS or L2TP 1, 2
>   troubleshooting 1
>   using in profiles 1, 2
> remote defect indication cells. See RDI cells
> remote loopback mode See OAM loopback mode
> remote loopback operation
>   halting
>     calculation and display of received data at the prompt 1
>     calculation and display of transmitted data at the prompt 1
>     viewing calculated loopback details 1
>   prerequisite for enabling remote peer to loop back PDUs 1
>   starting 1
>   stopping 1
> remote loopback request
>   error message
>     if local entity is not placed in loopback mode 1
>     if remote entity is not configured for loopback 1
>   Loopback control OAM PDU and 1
>   placing the interface of remote peer in loopback 1
>   received from the local entity
>     by the remote peer 1
> remote OAM entity
>   prerequisite for enabling loopback operation on 1
> remote OAM peer
>   Ethernet OAM link-fault management and 1
>   example scenario
>     for not building the OAM association 1
>   intentional discard of data frames
>     when loopback is enabled 1
>   notifying forwarding state
>     to local OAM entity 1
>   preventing both local and remote entities
>     from simultaneous loopback 1
>   receipt of Information PDUs
>     determination of OAM connection establishment 1
>     processing of configured rules on local entity details 1
>   supporting remote loopback
>     discarding locally sourced non-OAM PDUs 1
>     forwarding non-OAM PDUs to local entity 1
> round-robin packet distribution with MLPPP 1
> route interface command 1
> routing, configuring for transparent bridging 1
> RSTP (Rapid Spanning Tree Protocol) 1
>   Ethernet link redundancy 1, 2

S

> S-VLAN tags
>   virtual circuit identifier (VCI) mapping to
>     in ATM-to-Ethernet conversion 1
> S-VLANs (stacked virtual local area networks)
>   address possibilities 1
>   bridged Ethernet configurations 1
>   configuring PPPoE over S-VLAN 1
>   configuring to support dynamic PPPoE 1
>   configuring tunnel interfaces
>     advantages 1
>     example 1
>     interface stacking 1
>   displaying status 1, 2
>   oversubscription 1
>   overview 1
>   PPPoE over S-VLAN over bridged Ethernet 1
> scrambling ATM cell payload 1
> scripts
>   using to configure dynamic interfaces 1
> SDH (Synchronous Digital Hierarchy) 1, 2
> serial description command 1
> serial interfaces
>   configuring 1, 2, 3, 4, 5
> Serial Line Address Resolution Protocol. See SLARP
> service category, configuring for PVCs 1
> service name tables, PPPoE. See PPPoE service name tables
> SFPs (small form-factor pluggable transceivers) 1, 2
> short sequence number (SSN) header format 1
> show aaa commands
>   show aaa tunnel-parameters 1
> show atm commands
>   show atm aal5 interface 1, 2, 3
>   show atm atm1483 1
>   show atm bulk-config 1
>   show atm interface 1
>   show atm map 1, 2
>   show atm oam 1
>   show atm ping 1
>   show atm subinterface 1, 2, 3, 4
>   show atm vc 1, 2, 3
>   show atm vc atm 1
>   show atm vc-class 1
>   show atm vp 1
>   show atm vp-description 1
>   show atm vp-tunnel 1, 2, 3, 4
>   show nbma arp 1
> show bridge commands
>   show bridge 1
>   show bridge groups 1
>   show bridge interface 1
>   show bridge port 1
>   show bridge table 1
> show bridge1483 interface command 1
> show columns command 1, 2
> show frame-relay commands
>   show frame-relay interface 1, 2
>   show frame-relay lip 1
>   show frame-relay lmi 1, 2
>   show frame-relay map 1, 2
>   show frame-relay multilinkInterface 1
>   show frame-relay pvc 1, 2
>   show frame-relay subinterface 1, 2
>   show frame-relay summary 1, 2
> show hdlc interface command 1
> show interfaces commands
>   show interfaces fastEthernet 1, 2
>   show interfaces gigabitEthernet 1, 2
>   show interfaces lag 1
>   show interfaces lag members 1
>   show interfaces pos 1
>   show interfaces tenGigabitEthernet 1, 2
> show ip mac-validate command 1
> show mpls cross-connects atm command 1
> show ppp commands
>   show ppp interface 1
>   show ppp interface mlppp 1
>   show ppp interface summary 1, 2
> show pppoe commands
>   show pppoe interface 1, 2, 3
>   show pppoe interface lockout-time 1, 2
>   show pppoe interface summary 1
>   show pppoe subinterface 1, 2, 3
>   show pppoe subinterface summary 1
> show profile commands
>   show profile 1, 2, 3
> show radius commands
>   show radius override 1
>   show radius remote-circuit-id-delimiter 1
>   show radius remote-circuit-id-format 1
> show subscriber-policy command 1
> show vlan commands
>   show vlan bulk-config 1
>   show vlan subinterface 1, 2, 3
> show vlan subinterface command 1
> shutdown command 1
>   dynamic interfaces 1, 2
>   Frame Relay 1
>   POS 1
> shutting down interfaces
>   dynamic ATM 1483 1
>   dynamic VLAN 1
>   Frame Relay 1
>   POS 1
> Simple Network Management Protocol. See SNMP link status processing
> SLARP (Serial Line Address Resolution Protocol) 1, See also Cisco HDLC
>   Keep-Alive protocol 1
>   keepalive interval 1
>   overview 1
> slow protocols
>   bandwidth requirements 1
>   definition of
>     rate of transmission of OAM PDUs 1
>   multicast address of
>     and destination MAC address of remote entities 1
>   OAM messages and 1
> SMs (Service modules)
>   MLPPP features 1
> SNAP (subnetwork attachment point) 1
> SNMP (Simple Network Management Protocol) link status processing 1
> snmp trap frame-relay link-status command 1
> SONET (Synchronous Optical Network) 1, 2, 3
> source, clock
>   ATM interfaces 1
> SRP Ethernet interfaces
>   support for link-fault management 1
> SSN LCP (short sequence number Link Control Protocol) configuration option 1
> stacked virtual local area networks. See S-VLANs
> stateful SRP switchover
>   and atm atm1483 subscriber command 1
>   and subscriber command 1, 2, 3
>   Ethernet link-fault management
>     dependence on completion time 1
>     effect on OAM settings 1
>     of more than 2 seconds 1
>     recommendation for high and low threshold configuration 1, 2
>     recommendation for PDU loss threshold setting 1
> static interfaces 1, 2
>   configuring Multiclass MLPPP 1
>   creating in VC subranges 1, 2
>   creating in VLAN subranges 1
> static mapping, and NBMA interfaces 1
> subinterfaces
>   ATM 1483, dynamic 1
>   ATM 1483, static 1
>   Frame Relay, monitoring 1
>   MLFR, monitoring 1
>   VLAN, dynamic 1
> subnet mask
>   assigning to PPP interface 1
> subnetwork attachment point. See SNAP
> subranges, VC. See VC subranges
> subscriber command 1, 2, 3, 4, 5, 6, 7, 8, 9
> subscriber management, using for subscriber authentication 1, 2
> subscriber policies for transparent bridging 1, See also subscriber policy commands
>   configuring 1
>   defined 1
>   monitoring 1
> subscriber policy commands 1
>   arp 1
>   bridge subscriber-policy 1
>   broadcast 1
>   ip 1
>   multicast 1
>   pppoe 1
>   relearn 1
>   show subscriber-policy 1
>   subscriber-policy 1
>   unicast 1
>   unknown-destination 1
>   unknown-protocol 1
> subscribers
>   authenticating on dynamic bridged Ethernet interfaces 1, 2, 3
>   identifying for PPPoE 1
> support, technical See technical support
> SVC (switched virtual circuit)
>   ATM 1
>   Frame Relay 1, 2
> svlan commands
>   svlan ethertype 1, 2, 3, 4, 5, 6
>   svlan id 1
>     for S-VLAN tunnels 1
>     for standard S-VLANs 1, 2
> switch, 802.3ad 1
> switched virtual circuit. See SVC
> symbol errors
>   cumulative count of
>     threshold exceptions 1
>   detected using OAM link monitoring
>     for Ethernet interfaces 1
>   display of aggregated
>     in link event TLVs 1
>     in the show command output 1
>   enabling on IOAs that do not support
>     and events generation for that link 1
>   monitoring of
>     on IOAs that do not support 1
> symbol period errors
>   configuring
>     high threshold 1
>     low threshold 1
>     window 1
>   effect of configuration on
>     interfaces that do not support 1
>   exceeding threshold for
>     configuring LAG for removal of member link 1
>     configuring LAG to rebalance bundle 1
>   recommendation for configuring 1
> Synchronous Digital Hierarchy. See SDH
> Synchronous Optical Network. See SONET
> system
>   framing capabilities 1
> system clock
>   selecting clock source 1

T

> technical support
>   contacting JTAC 1
> terminated PPP session accounting statistics 1
> text and syntax conventions 1
> traffic management, ATM
>   types 1
> traffic-class
>   Multiclass MLPPP 1, 2
> traffic-shaping parameters 1
> transmit clock source, configuring
>   ATM interfaces 1
> transparent bridging. See bridging, transparent
> troubleshooting interfaces
>   dynamic PPP and PPPoE 1
>   PPP 1
>   PPPoE 1, 2
> TSMs (Tunnel Service modules)
>   MLPPP features 1

U

> ubr command 1, 2
> UNI (User-Network Interface) version 1, 2, 3, 4, 5
> unicast addressing 1
> unicast command 1
> unified ISSU
>   and Ethernet link-fault management 1
>   completion of
>     resumption of link-fault monitoring 1
>   in progress
>     halt of link-fault management 1
> Uniform Resource Locator messages. See URL messages
> unknown- commands
>   unknown-destination 1
>   unknown-protocol 1
> Unsupported OAM PDUs
>   viewing 1
> URL (Uniform Resource Locator) messages 1
> User-Network Interface. See UNI version

V

> vbr commands
>   vbr-nrt 1, 2
>   vbr-rt 1, 2
> VC (virtual channel)
>   integrity 1
>   per port, ATM 1
> VC (virtual circuit), monitoring 1
> VC classes
>   assigning to
>     ATM major interfaces 1
>     dynamic ATM 1483 subinterfaces 1, 2, 3
>     PVCs 1
>     static ATM 1483 subinterfaces 1
>   benefits 1
>   configuring 1
>   examples
>     configuration 1
>     precedence levels 1
>   monitoring 1
>   overview 1
>   precedence levels 1
>   upgrade considerations 1
> VC ranges, bulk configuration of
>   assigning VC classes 1, 2, 3
>   example 1
>   oversubscription 1, 2
>   overview 1
>   restarting LCP negotiations for PPPoA clients 1
> VC subranges
>   changing
>     adding to VC range 1
>     changing administrative state 1
>     configuring 1
>     merging 1
>     monitoring 1
>     overview 1
>     removing from VC range 1
>     shortening or expanding 1
>   creating static ATM interfaces in
>     configuring 1
>     monitoring 1
>     overview 1
>   overriding profile assignments 1, 2
>   oversubscription 1, 2
> vc-class atm command 1
> VCC (virtual channel connection) 1
> VCD (virtual circuit descriptor) 1, 2
> VCI (virtual channel identifier) 1, 2, 3
> vendor OUI TLV
>   component of Information OAM PDU
>     value of, usage 1
> vendor-specific attributes. See VSAs
> vendor-specific information
>   and Ethernet OAM link-fault management
>     Information OAM PDU component 1
>   format of, size of
>     usage 1
> Vendor-specific OAM PDUs
>   description of 1
> versions
>   UNI (User-Network Interface) 1, 2
> virtual channel connection. See VCC
> virtual channel identifier. See VCI
> virtual channel. See VC
> virtual circuit descriptor. See VCD
> virtual circuit identifier (VCI) tags
>   mapped to S-VLAN tags
>     in ATM-to-Ethernet conversion 1
> virtual circuit. See VC, monitoring
> virtual connections, ATM 1
> virtual local area networks. See VLANs
>   IPv4 and IPv6 over Dynamic PPPoE 1
> virtual path connection. See VPC
> virtual path descriptions, assigning 1
> virtual path identifier (VPI) tags
>   mapped to C-VLAN tags
>     in ATM-to-Ethernet conversion 1
> virtual path identifier. See VPI
> virtual path tunnels. See VP tunnels, ATM
> virtual path. See VP, monitoring
> virtual-router command 1
> vlan commands
>   encapsulation vlan 1
>   monitor vlan interface 1
>   profile vlan override 1
>   vlan advisory-rx-speed 1, 2
>   vlan advisory-tx-speed 1, 2
>   vlan auto-configure 1, 2
>   vlan auto-configure agent-circuit-identifier 1, 2
>   vlan bulk-config 1, 2, 3
>   vlan bulk-config modify 1
>   vlan bulk-config shutdown 1
>   vlan description 1, 2
>   vlan id 1, 2
>   vlan profile 1, 2
>   vlan service-profile 1
> VLAN subinterfaces
>   base profiles 1
>   nested profile assignments 1
>   overriding profile assignments 1
> VLAN subinterfaces, dynamic
>   benefits of using 1
>   bulk configuration of VLAN ranges 1
>   changing VLAN subranges 1, 2
>   configuring 1
>   configuring with agent-circuit-identifier information 1, 2
>   creating static VLAN interfaces in VLAN subranges 1
>   monitoring 1
>   overriding base profile assignments 1
>   overview 1
>   profiles for 1
> VLAN subranges
>   changing
>     adding to VLAN range 1
>     changing administrative state 1
>     configuring 1
>     merging 1
>     monitoring 1
>     overview 1
>     removing from VLAN range 1
>     shortening or expanding 1
>   creating static VLAN interfaces in
>     configuring 1
>     monitoring 1
> VLANs (virtual local area networks)
>   bridged Ethernet configurations 1
>   configuring 1
>   configuring dynamic subinterfaces for 1
>   configuring for dynamic IP 1
>   configuring for dynamic PPPoE 1
>   configuring IPv4 and IPv6 over dynamic PPPoE 1
>   configuring to support dynamic PPPoE 1
>   displaying status 1, 2
>   IP over VLAN over bridged Ethernet 1
>   monitoring 1
>   MPLS over VLAN over bridged Ethernet 1
>   overview 1
>   PPPoE over VLAN over bridged Ethernet 1
> VP (virtual path) tunnels, ATM
>   overview 1
>   per module assembly 1
>   traffic rate 1
> VP (virtual path), monitoring 1
> VPC (virtual path connection) 1
> VPI (virtual path identifier) 1, 2, 3
> VSAs (vendor-specific attributes)
>   DSL Forum 26-1 1
>   levels of CLI access 1
>   MLPPP Bundle Name 1

W

> warm router restart
>   preservation of
>     remote loopback enabling and disabling settings 1

X

> X.21/V.35 interfaces
>   MLPPP features 1
> XFPs (10-gigabit small form-factor pluggable transceivers) 1