Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Supported Interface Types for QoS Profiles
- Configuring a QoS Profile
- Configuring Shadow Nodes

# Supported Interface Types for QoS Profiles

Each QoS profile command begins with a keyword that designates an interface type.

Table 1 lists the interface types and the commands that you can use with them.

Table 1: Interface Types and Supported Commands

Interface Type | Queue | Node | Group | Shadow Node
--- | --- | --- | --- | ---
atm | ✓ | ✓ | ✓ | ✓
atm-vc | ✓ | ✓ | – | ✓
atm-vp | ✓ | ✓ | – | ✓
bridge | ✓ | ✓ | – | ✓
ethernet | ✓ | ✓ | ✓ | ✓
fr-vc | ✓ | ✓ | – | ✓
ip | ✓ | ✓ | – | ✓
ip-tunnel | ✓ | ✓ | – | ✓
ipv6 | ✓ | ✓ | – | ✓
l2tp-session | ✓ | ✓ | – | ✓
l2tp-tunnel | ✓ | ✓ | – | ✓
lsp | ✓ | ✓ | – | ✓
serial | ✓ | ✓ | ✓ | ✓
server-port | ✓ | ✓ | ✓ | ✓
svlan | ✓ | ✓ | – | ✓
vlan | ✓ | ✓ | – | ✓

#### Related Topics

- Supported Interface Types for QoS Profiles
- Configuring a QoS Profile
- Configuring Shadow Nodes

#### Published: 2010-06-16

Help
|
My Account
|
Log Out