# frame-relay interface-dlci ietf

#### Syntax

frame-relay interface-dlci dlci ietf

no frame-relay interface-dlci dlci

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Assigns a data-link connection identifier to a specified Frame Relay subinterface on the router or access server. The DLCI number identifies a virtual circuit. The no version removes this assignment.

#### Options

- dlci—DLCI number to be used on the specified subinterface to identify a virtual circuit in the range 16–1007

#### Mode

Subinterface Configuration

#### Related Topics

- Configuring Frame Relay Layer 2 Services in the JunosE BGP and MPLS Configuration Guide