# Index

Symbols A B C D E F G H I J K L M N O P Q R S T U V W X

Symbols

> --More-- prompt 1, 2, 3, 4, 5
> .cnf files 1, 2, 3, 4, 5, 6, 7, 8, 9
> .dmp files 1, 2, 3, 4
> .hty files 1, 2, 3
> .log files 1, 2
> .pub files 1, 2, 3
> .rel files 1, 2, 3
>   specifying for reboot 1, 2
> .scr files 1, 2, 3
> .sts files 1, 2, 3
> .txt files 1, 2, 3
> 3des-cbc encryption algorithm for SSH 1, 2
> ? command 1, 2, 3

A

> AAA (authentication, authorization, accounting)
>   configuring 1
> aaa commands
>   aaa accounting vr-group 1
>   aaa authentication enable default 1
>   aaa authentication login 1, 2
>   aaa domain-map 1, 2
>   aaa local database 1
>   aaa local username 1
>   aaa new-model 1
>   aaa profile 1
> AAA Profile Configuration mode 1, 2
> AAL5 layer (ATM) 1
> abbreviating keywords 1
> abbreviations and acronyms 1
> access and uplink methods 1
> access levels (CLI) 1
> access lists 1
>   for Telnet sessions 1
> access-class in command 1
> access-list command 1, 2
> adapter commands
>   adapter accept 1
>   adapter disable 1
>   adapter enable 1
>   adapter erase 1
> Address Family Configuration mode 1, 2
> address-family ipv4 command 1
> address-family vpnv4 command 1
> agent, SNMP 1, 2
> algorithm negotiation, SSH 1
> arrow keys 1, 2, 3
> assembly numbers, displaying for hardware 1
> assembly revisions, displaying for hardware 1
> assigning an IP address 1, 2, 3, 4
> ATM interfaces 1
> ATM VC Class Configuration mode 1, 2
> ATM VC Configuration mode 1, 2
> attributes, SNMP 1
> authentication
>   AAA 1
>   FTP server 1
>   hmac-md5 for SSH 1
>   hmac-sha1 for SSH 1
>   hmac-sha1-96 for SSH 1
>   new model AAA 1
>   SSH user 1
> authentication trap, SNMP 1
> authorization
>   AAA 1
> Automatic Commit mode 1
> automatic synchronization
>   disabling 1
>   enabling 1
> autoupgrade 1
> avp command 1

B

> B-RAS applications
>   overview 1
> B-RAS commands
>   aaa accounting vr-group 1
> backing up software configuration 1
> Backspace key 1
> backup router 1
> bandwidth
>   associated error messages 1
>   line modules 1
>   SRP modules 1
> bandwidth errors
>   troubleshooting 1
> bandwidth oversubscription
>   configuring 1
>   monitoring 1
>   overview 1
> bandwidth oversubscription command 1
> banner command 1
> banners
>   configuring 1
> baseline commands
>   baseline show-delta-counts 1
>   baseline snmp 1
> BGP (Border Gateway Protocol) 1
> blowfish-cbc encryption algorithm for SSH 1
> boot commands
>   boot backup 1
>   boot config 1
>   boot config factory-defaults 1
>   boot config once 1
>   boot config running-configuration 1
>   boot config startup-configuration 1
>   boot force-backup 1
>   boot hotfix 1
>   boot revert-tolerance 1
>   boot revert-tolerance never 1
>   boot subsystem 1
>   boot system 1
> Boot mode 1, 2
>   accessing 1
>   software installation 1
> booting the system 1, 2, 3, 4, 5
>   rebooting 1
>   while running scripts or macros 1
> Border Gateway Protocol. See BGP
> bottom-up approach to network configuration 1
> bridge commands
>   bridge subscriber-policy 1
> broadcasts, NTP 1
> bulk statistics, SNMP
>   collecting 1, 2
>   configuring
>     collectors and receivers 1
>     schemas 1
>   formatter 1
>   if-stats objects 1, 2, 3
>   mapping to MIBs and CLI 1
>   monitoring
>     collection statistics 1
>     schema statistics 1
> bulkstats commands 1, See also show bulkstats commands
>   bulkstats collector 1, 2, 3, 4
>   bulkstats collector collect-mode 1
>   bulkstats collector description 1
>   bulkstats collector interval 1
>   bulkstats collector max-size 1
>   bulkstats collector primary-receiver 1
>   bulkstats collector secondary-receiver 1
>   bulkstats collector single-interval 1
>   bulkstats file-format endOfLine-Lf 1
>   bulkstats interface-type 1
>   bulkstats interfaces description-format common 1
>   bulkstats receiver remote-name 1
>   bulkstats schema 1
>   bulkstats schema subtree 1
>   bulkstats schema subtree policy 1
>   bulkstats traps 1
>   bulkstats virtual-router-group 1

C

> caching, configuration 1
> capitalization. See case sensitivity
> case sensitivity 1
> channelized E1 interfaces
>   configuring 1
> channelized T1 interfaces
>   configuring 1
> channelized T3 interfaces
>   configuring 1
>   line rates 1
> characters on terminal screen, setting bits for 1, 2
> Classifier Group Configuration mode 1, 2
> clear commands
>   clear line 1
> CLI (command-line interface) 1
>   abbreviating keywords 1, 2
>   accessing 1
>   command modes. See command modes
>   context-sensitive help 1, 2
>   editing keys 1
>   editing on 1
>   logging in 1
>   pausing 1
>   system prompts 1
> CLI access levels, VSA descriptions 1, 2
> CLI command execution by macro file 1
> CLI messages
>   configuring 1
> CLI status indicator 1
> client, SNMP 1, 2
>   configuring access 1, 2
> clock 1
> clock commands 1
>   clock set 1
>   clock summer-time date 1
>   clock summer-time recurring 1
>   clock timezone 1
> cOCx/STMx interfaces
>   line rates 1
> coldStart, SNMP trap 1
> Color Mark Profile Configuration mode 1, 2
> color-mark-profile command 1
> command history keys 1
> command modes 1, 2
>   accessing 1
>   exiting 1, 2
> command-line interface. See CLI
> command-line prompts 1
> commands
>   abbreviating 1
>   editing on CLI 1
>   issuing from other command modes 1, 2, 3
>   listing available 1
>   pausing before executing 1
>   using 1
> commands for troubleshooting 1
> community table, SNMP
>   community name 1
>   configuring 1
>   IP access list 1
>   privilege levels 1
> community, SNMP 1, 2, 3
> configuration caching 1
> configuration file 1
>   running 1
> configuration modes. See command modes
> configuration tasks, general 1
> configuration, software 1, 2
> configure command 1, 2, 3
> configuring. See specific feature or protocol
> confirmations explicit command 1
> console
>   monitoring settings 1
>   password 1
>   restricting login 1
>   setting speed 1
> console lines
>   clearing 1
> contact person for SNMP server 1
> context-sensitive help 1, 2
> control flow monitoring 1
> Control Plane Configuration mode 1, 2, 3
> control plane security 1
> control-plane command 1
> controller commands 1
> Controller Configuration mode 1, 2
> conventions
>   notice icons 1
>   text and syntax 1
> copy commands
>   copy 1, 2, 3
>   copy running-configuration 1
>   copy running-configuration startup-configuration 1
>   copy startup-configuration 1
>   examples 1
> copying the software release file 1, 2, 3
> core dump files for troubleshooting 1, 2
> core dumps 1
> corrupted files. See flash cards, scanning
> crypto key dss command 1
> Ctrl-key combinations (CLI)
>   command history 1
>   command-line editing 1
> current configuration
>   saving 1, 2
> customer support 1
>   contacting JTAC 1
>   gathering information for 1

D

> data link-layer interfaces
>   configuring 1
> data set ready signal. See DSR
> data-character-bits command 1
> default version 1
> default virtual router 1
> delete command 1
> Delete key 1
> denial of service (DoS) 1
>   attaching groups 1
>   attacks 1
>   group parameters 1
>   protection 1
>   protocol mapping 1
> DHCP Pool Configuration mode 1, 2, 3
> diag command 1
> diag-level command 1
> diagnostics
>   enabling at warm restart 1
> Diffie-Hellman key exchange 1
> digital subscriber line access multiplexers. See DSLAMs
> dir command 1
> disable command 1, 2
> disable-autosync command 1
> disconnect ssh command 1
> display terminal
>   configuring 1
> displaying configuration information. See show commands
> distributed denial of service (DDoS) attack 1
> distribution lists 1
> DNS (Domain Name System) 1
>   configuring 1
> do command 1, 2, 3
> documentation set
>   comments on 1
> Domain Map Configuration mode 1, 2
> Domain Map Tunnel Configuration mode 1, 2
> DoS protection group commands
>   atm dos-protection-group 1
>   bridge1483 dos-protection-group 1
>   dos-protection-group 1
>   ethernet dos-protection-group 1
>   frame-relay dos-protection-group 1
>   hdlc dos-protection-group 1
>   ip dos-protection-group 1
>   ipv6 dos-protection-group 1
>   lag dos-protection-group 1
>   ppp dos-protection-group 1
>   pppoe dos-protection-group 1
>   priority burst 1
>   priority over-subscription-factor 1
>   priority rate 1
>   protocol burst 1
>   protocol drop-probability 1
>   protocol priority 1
>   protocol rate 1
>   protocol skip-priority-rate-limiter 1
>   protocol weight 1
>   use canned-group 1
>   vlan dos-protection-group 1
> Down Arrow key 1
> draft RFCs 1
> Drop Profile Configuration mode 1, 2
> drop-profile command 1
> DS1 channels 1
> DS3 channels 1
> DSLAMs (digital subscriber line access multiplexers) 1, 2, 3, 4
> DSR (data set ready), restricting login with 1
> dsr-detect command 1
> dump files, core 1

E

> E120 and E320 Broadband Services Routers
>   managing 1
> E3 interfaces
>   line rates 1
> E320 Broadband Services Routers
>   interface specifiers 1
> edge aggregation applications 1
>   private line aggregation 1
> editing on command-line interface 1
> enable commands
>   enable 1, 2, 3, 4
>   enable password 1
>   enable privilege-level 1
>   enable secret 1
> enable passwords, erasing 1
> encrypt passwords 1
> encryption
>   3des-cbc for SSH 1
>   blowfish-cbc for SSH 1
>   configuring SSH 1
>   twofish-cbc for SSH 1
> end command 1
> Enter key 1, 2, 3
> Enterprise SNMP MIB 1
> entity, SNMP 1
> environment, system 1
> erase secrets command 1, 2
> Esc-key combinations (CLI) 1
> Ethernet
>   Telnet on 1
> Ethernet port on SRP module 1
>   monitoring 1
> events
>   SNMP 1
> exception commands 1, See also show exception commands
>   exception dump 1
>   exception gateway 1
>   exception monitor 1
>   exception protocol ftp 1
>   exception source 1
> exclude-subsystem command 1
> exec-banner command 1
> exec-timeout command 1
> exit command 1, 2
> exiting the system 1
> Explicit Path Configuration mode 1, 2
> E Series routers 1
>   assigning IP address to 1
>   booting 1, 2, 3, 4
>   remote access. See B-RAS applications

F

> Fast Ethernet interfaces
>   specifying an interface 1
> file corruptions 1
> file system configuration, saving current 1
> files
>   copying 1, 2, 3
>   deleting 1
>   macro 1
>   managing 1
>   monitoring 1
>   redirecting 1
>   renaming 1
>   transferring 1
>   types of 1
>   viewing 1
> flash (NVS or nonvolatile storage) cards 1
>   copying 1
>   device names 1
>   different capacities 1
>   E120 and E320 Broadband Services Routers features 1
>   formatting 1
>   halt command to prevent corruption 1
>   installing 1
>   managing 1
>   monitoring 1
>   primary 1
>   rebooting and configuration data 1
>   rebooting in response to corrupt sectors 1
>   replacing 1
>   scanning
>     physical errors 1
>     structural errors in data 1
>   scanning utility 1
>   secondary 1
>   synchronizing 1
>   synchronizing with different capacities 1
>   validating and recovering file integrity 1
> flash-disk commands
>   flash-disk compare 1
>   flash-disk duplicate 1
>   flash-disk initialize 1
>   flash-disk scan 1
> Frame Relay interfaces 1
> FTP access 1, 2
>   configuring 1
> FTP client 1
> FTP server 1
>   authentication 1
>   configuring 1
>   monitoring 1
> ftp-server enable command 1

G

> Get operation, SNMP 1
> GetBulk operation, SNMP 1
> GetBulk PDU type, SNMP 1
> GetNext operation, SNMP 1
> GetNextRequest PDU type, SNMP 1
> GetRequest PDU type, SNMP 1
> GetResponse PDU type, SNMP 1
> Global Configuration mode 1, 2, 3
>   exiting 1
> group, SNMP 1

H

> halt command 1, 2
> hardware
>   monitoring information 1
>   standards 1
>   versions, displaying 1, 2
> HDLC parameters 1
> help 1
>   CLI system 1
> help command 1, 2, 3
> history command 1
> hmac-md5 authentication for SSH 1
> hmac-sha1 authentication for SSH 1
> hmac-sha1-96 authentication for SSH 1
> host command 1
> host ftp command 1
> host table, modifying 1, 2
> hostname command 1
> hotfix activate command 1
> hotfix files, monitoring 1
> hotfixes 1
>   activating 1
>   arming 1
>   backup settings and 1
>   compatibility 1
>   dependencies 1
>   displaying 1
>   hot-patchable 1
>   startup 1
>   synchronizing on SRP modules 1

I

> I/O adapters. See IOAs
> I/O modules
>   software compatibility 1
> if constructs, macro 1
> ILMI (integrated local management interface) 1
> image on primary SRP module, copying 1
> installing system software 1, 2
>   required information 1, 2, 3
> interactive help system. See help
> interface commands
>   interface 1, 2, 3
>   interface fastEthernet 1
>   interface loopback 1
> Interface Configuration mode 1, 2
> interfaces 1
>   configuring 1
>   Fast Ethernet 1
>   physical, configuring 1, 2
>   shared interfaces 1
>   subscriber interfaces 1
> IOA configurations
>   deleting 1, 2
> IOAs
>   disabling 1, 2
>   enabling 1
>   erasing configurations 1, 2
>   replacing 1
> IP access list, SNMP 1
> IP addresses
>   assigning 1, 2, 3
>   configuring 1
> ip commands
>   ip atm-vc 1
>   ip dhcp-local pool 1
>   ip domain-lookup 1, 2
>   ip domain-lookup transit-virtual-router 1
>   ip domain-name 1
>   ip ftp source-address 1
>   ip ftp source-interface 1
>   ip name-server 1
>   ip vrf 1, 2
> IP multicast 1
> IP NAT Pool Configuration mode 1, 2
> ip nfs commands
>   ip nfs 1
>   ip nfs host 1
> ip rate-limit-profile command 1
> ip ssh commands
>   ip ssh authentication-retries 1
>   ip ssh crypto 1
>   ip ssh disable-user-authentication 1
>   ip ssh mac 1
>   ip ssh sleep 1
>   ip ssh timeout 1, 2
> IP support
>   IP/ATM 1
>   IP/Ethernet 1
>   IP/FR 1
>   IP/HDLC 1
>   IP/PPP 1
> IP tunnels 1
> ip vrf commands
>   ip vrf 1
> IPSec (IP Security)
>   AH 1
>   ESP 1
> IPSec CA Identity Configuration mode 1
> ipsec commands
>   ipsec ca identity 1
>   ipsec identity 1
>   ipsec ike-policy-rule 1
>   ipsec key manual 1
>   ipsec key pubkey-chain rsa 1
> IPSec Identity Configuration mode 1, 2
> IPSec IKE Policy Configuration mode 1, 2
> IPSec Manual Key Configuration mode 1, 2, 3
> IPSec Peer Public Key Configuration mode 1, 2
> IPSec Transport Profile Configuration mode 1, 2
> IPSec Tunnel Profile Configuration mode 1
> IPv6 Local Configuration mode 1
> IPv6 Local Pool Configuration mode 1
> IS-IS protocol 1
> issuing commands from other CLI modes 1, 2, 3

J

> Juniper Networks E Series enterprise SNMP MIB 1

K

> keywords 1, 2
>   partial-keyword 1

L

> L2 Transport Load-Balancing-Circuit Configuration mode 1, 2
> L2C commands
>   l2c 1
>   neighbor 1
> L2TP (Layer 2 Tunneling Protocol) 1
> l2tp commands
>   l2tp destination profile 1
>   l2tp rate-limit-profile 1
>   l2tp switch-profile 1
> L2TP Destination Profile Configuration mode 1, 2
> L2TP Destination Profile Host Configuration mode 1, 2
> L2TP Tunnel Switch Profile Configuration mode 1, 2
> Layer 2 Control Configuration mode 1, 2
> Layer 2 Control Neighbor Configuration mode 1, 2
> Layer 2 Tunneling Protocol. See L2TP
> layered approach to network configuration 1
> LDP Configuration mode 1, 2
> Left Arrow key 1
> levels of CLI access 1
> line command 1, 2, 3
> Line Configuration mode 1, 2
> line module configurations
>   deleting 1, 2
> line modules
>   allowed combinations 1, 2
>   bandwidth 1
>   combinations 1, 2
>   disabling 1, 2
>   enabling 1
>   erasing configurations 1, 2, 3
>   initialization sequence 1
>   line rates 1
>   performance rate 1
>   replacing 1
>   restricted combinations 1
>   slot groups 1, 2, 3
>   software
>     compatibility 1
>   switch usage 1
>   troubleshooting 1
> line rates 1
> line vty command 1, 2
> lines
>   clearing 1
>   configuring 1
>   monitoring 1
>   setting on terminal screen 1
> link-up, link-down traps, SNMP 1
> linking to an FTP server. See FTP access
> listing commands available 1
> listing configuration settings. See show commands
> listing files on system 1
> LMI (local management interface) 1, 2, 3
> Local IPSec Transport Profile Configuration mode 1, 2, 3
> Local User Configuration mode 1, 2, 3
> location of SNMP server 1
> log commands 1
>   log severity 1
> logging in to system 1
> logging system events
>   viewing logs 1
> login banner 1
> login commands
>   login 1, 2, 3
>   login authentication 1
> login conditions
>   configuring 1
> long scripts, copying 1

M

> MAC (media access control) addresses
>   configuring for SSH 1
> macro (.mac) files 1, 2
> macro command 1
> macros
>   comments 1
>   conditional execution 1
>   control expressions 1
>   environment commands 1
>   if constructs 1
>   invoking from another macro file 1, 2
>   literals 1
>   naming 1
>   noncontrol expressions 1
>   operators 1
>     arithmetic 1
>     assignment 1
>     extraction 1
>     increment and decrement 1
>     logical 1
>     miscellaneous 1
>     relational 1
>     string 1
>   resetting system while running 1
>   variables 1
>   while constructs 1
>   writing 1, 2
> managed object, SNMP 1
> Management Information Bases. See MIBs
> Manual Commit mode 1
> manuals
>   comments on 1
> Map Class Configuration mode 1, 2
> Map List Configuration mode 1, 2
> map-class frame-relay command 1
> map-list command 1
> master router 1
> master, NTP 1
> MD5 authentication
>   SSH 1
> memory (hardware), displaying 1
> memory management 1
> memory warning command 1
> message authentication code. See MAC addresses
> message-of-the-day (MOTD) banner 1, 2
> MIBs (Management Information Bases)
>   definition of 1
>   Juniper Networks E Series enterprise 1
>   standard SNMP 1
> modules
>   disabling 1
>   E Series, managing 1
>   E120 and E320 Broadband Services Routers 1
>   enabling 1
>   monitoring 1
>   replacing 1
> monitor. See terminal
> more command 1
> motd-banner command 1
> mount command 1
> mounting a CD on an FTP server 1, 2, 3
> MPLS (Multiprotocol Label Switching) 1
> mpls commands
>   mpls explicit-path name 1
>   mpls ldp profile 1
>   mpls rsvp profile 1
>   mpls tunnels profile 1
> Multiprotocol Label Switching. See MPLS

N

> names
>   renaming local files 1
>   system name 1
> network configuration 1
>   layered (bottom-up) approach 1
>   routing protocols 1
> network elements, SNMP 1
> Network File System. See NFS client
> network planning 1
>   access lists 1
>   BGP 1
>   COCX-F3 modules 1
>   configurable HDLC parameters 1
>   configuration overview 1, 2
>   CT3 12-F0 modules 1
>   data link-layer interfaces 1
>   distribution lists 1
>   E3 modules 1
>   Ethernet modules 1
>   general configuration tasks 1
>   interfaces and subinterfaces 1
>   IP multicast 1
>   IP/ATM 1
>   IP/Frame Relay 1
>   IP/HDLC 1
>   IP/PPP 1
>   L2TP 1
>   layered approach 1
>   line module features 1
>   MPLS 1
>   non-PPP equal access 1
>   OSPF 1, 2
>   physical layer interfaces 1
>   policy management
>     configuring 1
>   private line aggregation 1
>   RIP 1
>   route maps 1
>   routing policy 1
>   routing protocols 1
>   SONET 1
>   virtual routers 1
>   VRRP 1
> network servers, displaying list of 1
> Network Time Protocol. See NTP
> new model AAA authentication 1
> NFS client
>   configuring 1
>   overview 1
> no boot hotfix all-releases command 1
> no command 1, 2
> non-PPP equal access 1
> nonvolatile storage. See flash (NVS or nonvolatile storage) cards
> notice icons 1
> NTP (Network Time Protocol)
>   best server 1
>   broadcasts 1
>   client-server associations 1
>   configuring 1
>   master 1
>   monitoring 1, 2
>   overview 1
>   peers 1
>   replies 1
>   requests 1
>   servers 1, 2, 3
>   synchronization 1
>   virtual routers 1, 2
> NTP client
>   configuring the system as 1
>   system operation as 1
> ntp commands 1, See also show ntp commands
>   ntp access-group 1
>   ntp broadcast 1
>   ntp broadcast-client 1
>   ntp broadcast-delay 1
>   ntp disable 1
>   ntp enable 1
>   ntp master 1
>   ntp server 1
>   ntp server enable 1
>   ntp source 1
> NTP control queries 1
> NTP servers
>   assigning 1
>   best 1
>   choosing 1
>   configuring virtual routers as 1
>   enabling NTP broadcasting 1
>   enabling on a virtual router 1
>   primary 1
>   selecting 1
>   system operation as 1

O

> objects, tracking reachability 1, 2, 3
> OC48/STM16 interfaces, configuring 1
> OCx/STMx interfaces
>   configuring 1
> Open Shortest Path First. See OSPF
> OSPF (Open Shortest Path First) 1
> output filtering
>   from the --More-- prompt 1
>   show command 1
> oversubscription, bandwidth
>   configuring 1
>   monitoring 1
>   overview 1
> overview, NTP 1

P

> packet mirroring
>   and SNMP 1
> packet size, SNMP 1
> pagination keys 1
> parameters 1, 2
> parent-group command 1, 2, 3
> partial releases, copying 1
> password command 1, 2, 3, 4
> passwords 1, 2, 3, 4, See also Privileged Exec mode
>   enabling 1
>   encryption 1
>   erasing console passwords 1
> passwords and secrets
>   deleting 1
> patching the system with hotfixes 1
> pausing before command execution 1
> PDU (protocol data unit) 1
> performance rate, line modules 1, 2
>   configuring 1
> physical errors in flash cards 1
> physical interfaces, configuring 1, 2
> physical slots
>   rebooting selected 1
> ping command 1, 2
> platform considerations
>   installing JunosE Software 1
>   macros 1
>   managing modules 1
>   network planning 1
>   passwords and security 1
>   SNMP 1
>   system booting 1
>   system clock 1
>   system management 1
>   using the CLI 1
>   virtual routers 1
> Policy List Configuration mode 1, 2
> Policy List Parent Group Configuration mode 1, 2, 3, 4, 5, 6, 7, 8, 9
> policy management 1
>   QoS classification and marking 1
>   rate limiting 1
>   types of services 1, 2
>   xDSL session termination 1
> polling NTP servers 1
> POS interfaces 1
> PPP (Point-to-Point Protocol)
>   protocol support 1
> PPPoE Service Name Table Configuration mode 1, 2
> pppoe-service-name-table command 1
> primary flash card
>   initializing 1
>   reformatting 1
> primary NTP servers 1
> private line aggregation 1
> privilege groups 1
> privilege level
>   accessing 1
>   ambiguous commands 1
>   changing command privileges 1
>   command exceptions 1
>   defining CLI 1
>   keyword mapping 1
>   password encryption 1
>   setting
>     default line 1
>     multiple commands 1
>     no or default versions 1
>   SNMP 1
>   viewing information 1
> privilege level command 1
> Privileged Exec mode 1, 2, 3, 4, 5, 6, See also passwords
>   accessing 1, 2, 3, 4, 5, 6
>   exiting 1, 2, 3
> privileged-level access (CLI) 1, 2, 3, See also Privileged Exec mode
> profile commands
>   profile 1
> Profile Configuration mode 1, 2
> progress indicator (CLI) 1
> prompts, CLI system 1
> protocol data unit. See PDU
> proxy, SNMP 1, 2
> pvc command 1

Q

> QoS (quality of service) 1
> QoS commands
>   qos-profile command 1
> QoS Interface Set Configuration mode 1, 2
> QoS Interface Superset Configuration mode 1, 2
> QoS Parameter Configuration mode 1
> QoS Parameter Definition Configuration mode 1, 2
> QoS Profile Configuration mode 1, 2
> QoS Shared Shaper Control Configuration mode 1
> qos-profile command 1
> qos-shared-shaper-control command 1
> Queue Profile Configuration mode 1, 2
> queue-profile command 1

R

> RADIUS (Remote Authentication Dial-In User Service)
>   authentication, restricting access 1
>   password authentication 1
>   per-user enable authentication 1
>   restricting access to commands 1, 2
>   user authentication 1
> radius commands
>   radius accounting server 1
>   radius authentication server 1
>   radius dynamic-request server 1
> RADIUS Configuration mode 1, 2
> radius relay commands
>   radius relay accounting server 1
>   radius relay authentication server 1
> RADIUS Relay Configuration mode 1
> Rate Limit Profile Configuration mode 1, 2
> rate limiting
>   per priority 1
>   per protocol 1
> reachability, tracking 1
> reaching an FTP server. See FTP access
> reboot history (reboot.hty) file 1
> reboot history, displaying 1
> rebooting the system 1, 2
> redistribute routes 1
> Redundancy Configuration mode 1, 2
> references
>   draft RFCs 1
>   hardware standards 1
>   non-RFC software standards 1
>   RFCs 1
> refusing NTP broadcasts 1
> regular expressions 1, 2
>   metacharacters 1
>     specifying as literals 1
> releasing available memory 1
> reload commands
>   reload 1, 2
>   reload at 1
>   reload in 1
>   reload slot 1
> Remote Authentication Dial-In User Service. See RADIUS
> remote host command 1
> Remote Neighbor Configuration mode 1, 2
> remote-neighbor command 1
> rename command 1
> renaming files 1
> replies, NTP 1
> reset button, software 1
> resetting while running scripts or macros 1
> resource commands
>   resource if-type 1
>   resource threshold 1
> resources
>   monitoring 1
> revisions, displaying assembly 1
> RFC 1213 interface numbering 1
> RFCs 1
>   draft 1
> Right Arrow key 1
> RIP (Routing Information Protocol) 1
> Route Map Configuration mode 1, 2
> route maps 1
> route-map command 1
> router commands
>   router 1
>   router bgp 1
>   router ospf 1
>   router pim 1
>   router rip 1, 2
> Router Configuration mode 1, 2
> routers. See system
> Routing Information Protocol. See RIP
> routing policy
>   configuring 1
> routing protocols 1
>   configuring 1
> routing, IP
>   configuring other protocols 1
>   monitoring 1
> RSVP Configuration mode 1, 2
> rtr commands
>   rtr 1
> RTR Configuration mode 1, 2
> run command 1, 2, 3

S

> schedule-profile command 1
> Scheduler Profile Configuration mode 1, 2
> screen. See terminal
> script files 1
> scripts
>   resetting system while running 1
> secondary NTP servers 1
> secure IP tunnels 1
> Secure Shell Server protocol. See SSH
> security
>   administration through SSH instead of Telnet 1
>   SSH issues 1
> security features of SNMP 1
> send command 1
> sending messages to terminals 1
> serial numbers, displaying for hardware 1
> servers, NTP 1
> service commands
>   service 1
>   service ctrl-x-reboot 1, 2
>   service manual-commit 1
>   service password-encryption 1, 2
>   service unattended password-recovery 1
> Service Manager commands
>   service-management service-session-profile 1
> Service Session Profile Configuration mode 1, 2
> Set operation, SNMP 1
> SetRequest PDU type, SNMP 1
> SFMs (switch fabric modules)
>   accepting configurations 1
>   disabling 1, 2
>   enabling 1
>   erasing configurations 1
>   overview 1
>   replacing 1
> shared interfaces 1
> show aaa commands
>   show aaa domain-map 1
> show bandwidth oversubscription 1
> show boot command 1
> show bulkstats commands 1
>   show bulkstats 1
>   show bulkstats collector interface-type 1
>   show bulkstats collector interval 1
>   show bulkstats collector max-size 1
>   show bulkstats collector transfer-mode 1
>   show bulkstats receiver 1
>   show bulkstats router-group 1
>   show bulkstats statistics 1
>   show bulkstats traps 1
> show command output, filtering 1
> show commands 1, 2
>   show output filtering feature 1, 2
>   show policy-list 1
>   show redirecting output 1
> show configuration commands 1
>   show configuration 1, 2
>   show configuration category 1
>   show configuration interface 1
>   show configuration virtual-router 1, 2
> show dos-protection-group 1
> show environment command 1
> show exception commands
>   show exception dump 1
>   show exception monitor 1
> show fabric weights command 1
> show flash command 1
> show ftp-server command 1
> show hardware command 1, 2
> show hosts command 1
> show hotfix command 1
> show ip commands
>   show ip domain-lookup command 1
>   show ip forwarding-table slot 1
>   show ip ssh 1
> show ip nfs command 1
> show last-reset command 1
> show line console 0 command 1
> show line vty command 1, 2
> show log commands
>   show log data 1
> show ntp commands
>   show ntp associations 1
>   show ntp associations detail 1
>   show ntp status 1
> show nvs command 1
> show processes command 1, 2
> show reboot-history command 1
> show reload command 1
> show running-configuration command 1, 2
> show secrets command 1
> show snmp commands
>   show snmp 1
>   show snmp community 1
>   show snmp interfaces 1
>   show snmp notificationLog 1
>   show snmp trap 1
>   show snmp trapstat 1
> show subsystems command 1
> show suspicious-control-flow-detection commands
>   show suspicious-control-flow-detection counts 1
>   show suspicious-control-flow-detection flows 1
>   show suspicious-control-flow-detection info 1
>   show suspicious-control-flow-detection protocol 1
> show tech-support command 1
> show terminal command 1, 2
> show timing command 1
> show users command 1
> show utilization command 1, 2
> show version command 1, 2, 3, 4
> show virtual-router command 1
> Simple Network Management Protocol. See SNMP
> sleep command 1
> slot commands
>   slot accept 1
>   slot disable 1
>   slot enable 1
>   slot erase 1, 2
> slot groups and module arrangements 1, 2
> SNMP (Simple Network Management Protocol) 1
>   agent software 1, 2
>   attributes 1
>   bulk statistics collection 1
>   client software 1, 2
>     configuring access 1, 2
>   communities 1, 2, 3
>   compressing interfaces 1
>   configuration tasks 1
>   enabling 1
>   encoding method 1
>   engine 1
>   entity 1
>   group 1
>   interface numbering 1
>   management features 1
>   managing interface sublayers 1
>   memory warning 1
>   monitoring interface tables 1
>   monitoring status 1, 2
>   multiple virtual routers 1, 2
>   operations 1
>   packet mirroring 1
>   packet size, setting 1
>   PDU 1
>   proxy, creating 1
>   RFC 1213 compatibility 1
>   schema
>     configuring 1
>     monitoring 1
>   security features 1
>   server 1
>   server parameters, setting 1
>   traps. See SNMP traps
>   users, configuring 1
>   versions 1
>   view 1, 2
>   viewing status 1
>   virtual routers 1
> SNMP commands 1, See also bulkstats commands
>   agent context-name 1
>   bulkstats interfaces rfc 1213 1
>   delta-sampling 1
>   enable 1
>   event 1
>   frequency 1
>   notification id 1
>   resource 1
>   trigger 1
> snmp commands
>   snmp interfaces description-format 1
>   snmp trap ip link-status 1
>   snmp trap link-status 1
>   snmp-server 1
>   snmp-server community 1
>   snmp-server contact 1
>   snmp-server enable traps 1
>   snmp-server host 1, 2, 3
>   snmp-server interfaces compress 1
>   snmp-server interfaces compress-restriction 1
>   snmp-server interfaces rfc1213 1
>   snmp-server location 1
>   snmp-server notificationLog ageOut 1
>   snmp-server notificationLog entryLimit 1
>   snmp-server notificationLog log 1
>   snmp-server packetsize 1
>   snmp-server trap-proxy 1
>   snmp-server trap-source 1
>   snmp-server user 1
> SNMP Event Manager Configuration mode 1, 2
> SNMP traps 1, 2, 3
>   enabling 1
> software
>   compatibility 1
>   configuration 1, 2
>     backing up 1
>     saving 1
>   installing 1, 2
>   line rates 1
>   release file 1
>   updating 1
>   upgrading 1, 2, 3
> software release file 1
>   accessing 1, 2, 3
>   specifying for reboot 1
> software reset button 1
> software standards
>   draft RFCs 1
>   non-RFC standards 1
>   RFCs 1
> software versions, displaying 1, 2
> Space key 1, 2
> speed command 1
> SRP module configurations
>   deleting 1, 2
> SRP module redundancy
>   hotfixes and 1
>   validating and recovering file integrity 1
> SRP modules
>   bandwidth 1
>   configuring 1
>   copying image 1
>   core dump file 1
>   disabling 1
>   enabling 1
>   erasing configurations 1, 2
>   overview 1
>   removing 1
>   replacing 1
>   reset button 1
>   synchronizing 1
> SSH (Secure Shell Server) 1
>   algorithm negotiation 1
>   client configuration 1
>   configuration prerequisites 1
>   configuring 1
>   connections 1
>   disabling 1
>   enabling 1
>   encryption algorithms
>     3des-cbc 1
>     blowfish-cbc 1
>     twofish-cbc 1
>   encryption, configuring 1
>   generating host keys 1
>   host key management 1
>   key exchange 1
>   message authentication
>     configuring 1
>     hmac-md5 1
>     hmac-sha1 1
>     hmac-sha1-96 1
>   monitoring 1
>   performance issues 1
>   security concerns 1
>   server public key files 1
>   terminating 1
>   user authentication 1
>     configuring 1
>   user key management 1
> standards
>   draft RFCs 1
>   hardware standards 1
>   non-RFC software standards 1
>   RFCs 1
> startup configuration
>   saving 1
> static host maps, adding 1, 2
> static tunnels 1
> statistics
>   SNMP 1, 2
> statistics (.sts) files 1
> Statistics Profile Configuration mode 1, 2
> statistics-profile command 1
> status indicator (CLI) 1
> stratum 1 servers. See NTP servers, primary
> structural errors in flash data 1
> Subinterface Configuration mode 1, 2
> subinterfaces 1, 2
>   configuring 1
> subscriber interfaces 1
> subscriber policy commands
>   subscriber-policy 1
> Subscriber Policy Configuration mode 1, 2
> summer time, specifying 1
> support, technical See technical support
> suspicious control flow detection 1
>   display options 1
>   logs 1
>   parameters 1
>   traps 1
> suspicious control flow monitoring 1
> suspicious-control-flow-detection commands
>   baseline suspicious-control-flow-detection counts 1
>   clear suspicious-control-flow-detection 1
>   suspicious-control-flow-detection grouping-off 1
>   suspicious-control-flow-detection off 1
>   suspicious-control-flow-detection protocol backoff-time 1
>   suspicious-control-flow-detection protocol low-threshold 1
>   suspicious-control-flow-detection protocol threshold 1
> switch fabric modules. See SFMs
> switch usage, line modules 1
> synchronization process 1, 2
> synchronization reserve file 1
> synchronize command 1, 2
> system
>   autoupgrade feature 1
>   basic parameters 1
>   booting 1, 2
>     rebooting 1
>   command-line interface. See CLI
>   configuring automatically 1
>   environment information 1
>   exiting 1
>   FTP client 1
>   FTP server 1
>   initializing line modules 1
>   levels of access 1, 2
>   logging in 1
>   logging/troubleshooting, commands for 1, 2
>   managing 1
>   monitoring 1
>   passwords 1
>   patching with hotfixes 1
>   physical slots, rebooting 1
>   RADIUS password authentication 1
>   software reset button 1
>   system configuration files 1, 2
>   system name 1
>   TFTP client 1
>   timing 1
>   updating with hotfixes 1
>   virtual router limitations 1
> system clock
>   setting 1
> system commands
>   privilege 1
>   privilege-group alias 1
>   privilege-group membership 1
>   privilege-group membership clear 1
>   write core 1
> system configuration
>   saving current 1, 2, 3
>   saving startup 1
> system passwords. See passwords
> system security 1
> system.log file 1

T

> T1 lines, controllers for 1
> T3 interfaces
>   configuring 1
>   controllers for 1
>   line rates 1
> Tab key 1, 2, 3
> TACACS+
>   aaa authentication login 1
>   restricting access to commands 1
> tag-group command 1
> tech-support encoded-string command 1
> technical support
>   contacting JTAC 1
> Telnet
>   access lists 1
>   client, using 1
>   configuring to listen in nondefault virtual router 1
>   logins 1
> telnet commands
>   telnet 1
>   telnet listen 1
> terminal
>   configuring display 1
>   displaying configuration 1
>   displaying international characters 1, 2
>   sending messages to 1
>   setting length (in lines) 1
>   setting width (in characters) 1
> terminal commands 1, See also show terminal command
>   terminal data-character-bits 1
>   terminal length 1
>   terminal speed 1
>   terminal width 1
> text and syntax conventions 1
> text files 1
> TFTP client 1
> thermal protection mode 1
> time limits, setting
>   for user input 1
>   for user login 1
> time zone, specifying 1
> timeout login response command 1
> timing commands
>   timing disable-auto-upgrade 1
>   timing select 1
>   timing source 1
> timing, system 1, See also system clock
>   configuring 1
>   monitoring 1
> trace command 1
> tracking objects 1, 2, 3
> Traffic Class Configuration mode 1, 2
> Traffic Class Group Configuration mode 1, 2
> traffic-class command 1
> traffic-class-group command 1
> transport protocols, xDSL 1
> traps command 1
> traps, SNMP
>   categories 1
>   configuring 1
>   configuring notification logs for 1
>   configuring trap queues 1
>   operation 1
>   PDU type 1
>   recovering lost traps 1
>   severity levels 1
>   specifying an egress point for 1
>   statistics 1
>   status information 1
> troubleshooting core dump files 1
> tunnel commands
>   tunnel 1, 2
> Tunnel Group Configuration mode 1, 2, 3
> Tunnel Group Tunnel Configuration mode 1, 2, 3
> Tunnel Profile Configuration mode 1, 2
> Tunnel Server Configuration mode 1, 2
> tunnel-server command 1
> tunnels, IP 1
> twofish-cbc encryption algorithm for SSH 1

U

> Universal Coordinated Time. See UTC
> Up Arrow key 1
> updating the system software 1
> updating the system with hotfixes 1
> upgrading software
>   systems with one SRP module 1
>   systems with two SRP modules 1
> uplink methods 1
> user access, restricting 1
> user authentication, configuring 1, 2, See also authentication
> User Exec mode 1, 2, 3, See also Privileged Exec mode
> user interface commands 1
> user interface, customizing 1
> user level access (CLI) 1
> UTC (Universal Coordinated Time) 1, 2

V

> vc-class atm command 1
> vendor-specific attributes. See VSAs
> versions
>   default 1
>   displaying for hardware 1
>   displaying for hardware/software 1
>   displaying for software 1
>   SNMP 1
> view, SNMP 1, 2
> viewing files 1, 2, See also show commands
> virtual interfaces (subinterfaces) 1
> virtual router commands
>   ip vrf 1
>   virtual-router 1, 2, 3, 4
> Virtual Router Redundancy Protocol (VRRP). See VRRP
> virtual routers 1, 2
>   configuring 1, 2
>   default virtual router 1
>   map VR to domain map 1, 2
>   monitoring 1, 2
>   name resolvers for multiple 1
>   NTP 1, 2, 3, 4
>   restricting access 1
>   SNMP 1, 2
>     managing 1
>   VPNs 1
>   VRFs 1
>   VSAs 1
>   with routing protocols 1, 2, 3
> VPN routing and forwarding instance. See VRF
> VPNs (virtual private networks) 1
> VR Group Configuration mode 1, 2
> VRF (VPN routing and forwarding instance) 1
> VRF Configuration mode 1, 2
> VRRP (Virtual Router Redundancy Protocol) 1, 2
> VSAs (vendor-specific attributes)
>   levels of CLI access 1
>   restricting access to virtual routers 1
> vty lines
>   clearing 1
>   configuring 1
>   managing 1
>   monitoring 1
>   users of 1

W

> waiting before command execution 1
> warm restart
>   enabling diagnostics at 1
> warmStart, SNMP trap 1
> while constructs, macro 1
> width of terminal screen, setting 1
> write memory command 1
> writing macros 1

X

> xDSL
>   protocols 1
>   session termination 1