Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# set dhcp relay max-client-packet-rate

#### Syntax

[ no ] set dhcp relay max-client-packet-rate [ packetsPerSecond ]

#### Release Information

Command introduced in JunosE Release 11.2.0.

#### Description

Configures DHCP relay to limit the maximum number of client packets that DHCP relay processes per second. The no version returns to the default, in which DHCP relay processes 4096 packets per second.

#### Options

- packetsPerSecond—Number of client packets that are processed per second in the range 0–4096.

#### Mode

Global Configuration

#### Published: 2010-07-14

Help
|
My Account
|
Log Out