Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

# radius connect-info-format

#### Syntax

radius connect-info-format { l2tp-connect-speed |
l2tp-connect-speed-rx-when-equal }

no radius connect-info-format

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the format of RADIUS attribute 77, Connect-Info, on the LNS. The format uses the received L2TP connect-speed AVPs that the LAC sends to the LNS. The no version restores the default, in which the LNS does not generate the Connect-Info attribute.

#### Options

- l2tp-connect-speed—Specifies that the Connect-Info attribute include only the RX speed when the RX speed is different from the TX speed and is greater than zero.
- l2tp-connect-speed-rx-when-equal—Specifies that the Connect-Info attribute always include the RX speed when the speed is greater than zero.

#### Mode

Global Configuration

#### Published: 2010-07-13

Help
|
My Account
|
Log Out