# tunnel-server

#### Syntax

[ no ] tunnel-server interfaceSpecifier

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the location of a dedicated or shared tunnel-server port on a module and accesses Tunnel Server Configuration mode, which enables you to provision the maximum number of tunnel-service interfaces to be used on the tunnel-server port. The default version restores the default configuration. On dedicated tunnel-server ports, the default configuration is the maximum number of tunnel-service interfaces that the tunnel-service module supports. On shared tunnel-server ports, the default configuration is zero tunnel-service interfaces provisioned. The no version unprovisions the tunnel-server port by reducing the number of provisioned tunnel-service interfaces to zero.

#### Options

- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers; port number specified must have the tunnel-server port assigned to it

#### Mode

Global Configuration

#### Related Topics

- Configuring QoS for Tunnel-Server Ports for L2TP LNS Sessions