# Monitoring Chassis-wide Configuration for L2TP Dial-out

#### Purpose

To display the chassis-wide configuration, operational state, and statistics for L2TP dial-out.

This command displays aspects of the dial-out state machine and details about the dial-out routes themselves. This section presents sample output. The actual output on your router may differ significantly.

#### Action

To display chassis-wide configuration, operational state, and statistics for L2TP dial-out:

    host1#show l2tp dial-out
    Operational status: inService
    Connecting timer value: 30 seconds
    Dormant timer value: 300 seconds

To display detailed chassis-wide configuration information:

    host1#show l2tp dial-out detail
        Dial-out Chassis Configuration and Operational Status
          Chassis operational status :   inService
          Dormant timeout            :   30 seconds
          Connecting timeout         :   30 seconds

    Dial-out Chassis Statistics
      Current sessions:                                0
      Maximum sessions:                                0
      Current sessions in the process of connecting:   0
      Maximum sessions connecting at one time:         0
      Current sessions pending:                        0
      Maximum sessions pending:                        0
      Current targets inhibited:                       0
      Maximum targets inhibited:                       0
      Authentication grant for nonexistent session:    0
      Authentication deny for nonexistent session:     0

    Dial-out Virtual router statistics
      Virtual routers active:                        0
      Virtual routers created:                       0
      Virtual routers removed:                       0
      Virtual routers in init-pending state:         0
      Virtual routers in init-failed state:          0
      Virtual routers in down state:                 0
      Virtual routers in in-service state:           0
      IP Discarded trigger frames:                   0
      Trigger frames received for unknown route:     0
      Sessions in dormant state:                     0
      Sessions in pending state:                     0
      Sessions in authenticating state:              0
      Sessions in connecting state:                  0
      Sessions in in-service state:                  0
      Sessions in inhibited state:                   0
      Sessions in post-inhibited state:              0
      Sessions in failed state:                      0

    Dial-out target statistics
      Targets active:                                0
      Targets created:                               0
      Targets removed:                               0
      Targets in down state:                         0
      Targets in inhibited state:                    0
      Targets in in-service state:                   0
      Triggers discarded:                            0
    Dial-out session statistics
      Sessions active:                               0
      Sessions created:                              0
      Sessions removed:                              0
      Sessions reset:                                0
      Triggers received:                             0
      Triggers enqueued:                             0
      Triggers discarded:                            0
      Triggers forwarded:                            0
      Triggers max enqueued:                         0
      Authentication requests:                       0
      No resources for authentication:               0
      Authentication grants:                         0
      Authentication Denies:                         0
      Dial-outs requested:                           0
      Dial-outs rejected:                            0
      Dial-outs established:                         0
      Dial-outs timed out:                           0
      Dial-outs torn down:                           0

To display summary information for chassis-wide configuration:

    host1#show l2tp dial-out summary
          Virtual routers in init pending state :              0
          Virtual routers in init failed state  :              0
          Virtual routers in down state         :              0
          Virtual routers in inService state    :              0
          Targets in down state                 :              0
          Targets in inhibited state            :              0
          Targets in inService state            :              0
          Sessions in dormant state             :              0
          Sessions in pending state             :              0
          Sessions in authenticating state      :              0
          Sessions in connecting state          :              0
          Sessions in inService state           :              0
          Sessions in inhibited state           :              0
          Sessions in postInhibited state       :              0
          Sessions in failed state              :              0

To display information about the operational or administrative state:

    host1#show l2tp dial-out state inService

#### Meaning

Table 94 lists the show l2tp dial-out command output fields.

Table 94: show l2tp dial-out Output Fields

Field Name | Field Description
--- | ---
Operational status | Current operational status of the chassis
Connecting timer value | Configuration of the connecting timeout
Dormant timer value | Configuration of the dormant timeout
Dial-out Chassis Statistics | Statistics at the chassis level
Current sessions | Total number of session currently active on the chassis
Maximum sessions | Highest value of current sessions recorded on the chassis since the last router restart
Current sessions in the process of connecting | Sessions currently in the connecting state
Maximum sessions connecting at one time | Highest number of sessions recorded on the chassis at the same time since the last router restart
Current sessions pending | Sessions in the pending state
Maximum sessions pending | Highest number of sessions recorded in the pending state since the last router restart
Current targets inhibited | Targets currently in the inhibited state
Maximum targets inhibited | Highest value of targets recorded in the inhibited state since the last router restart
Authentication grant for nonexistent session | Number of authentication requests granted to nonexistent sessions
Authentication deny for nonexistent session | Number of authentication requests denied to nonexistent sessions
Dial-out Virtual router statistics | Statistics at the virtual router level
Virtual routers active | VRs in use by the state machine
Virtual routers created | VRs that have been used by the state machine
Virtual routers removed | VRs no longer used by the state machine
Virtual routers in init-pending state | VRs in the initializationPending state
Virtual routers in init-failed state | VRs in the initializationFailed state
Virtual routers in down state | VRs in the down state
Virtual routers in in-service state | VRs in the inService state
IP Discarded trigger frames | Trigger frames that IP discarded
Trigger frames received for unknown route | Trigger frames received for an unknown route
Sessions in dormant state | Sessions on the VR that are in the dormant state
Sessions in pending state | Sessions on the VR that are in the pending state
Sessions in authenticating state | Sessions on the VR that are in the authenticating state
Sessions in connecting state | Sessions on the VR that are in the connecting state
Sessions in in-service state | Sessions on the VR that are in the inService state
Sessions in inhibited state | Sessions on the VR that are in the inhibited state
Sessions in post-inhibited state | Sessions on the VR that are in the postInhibited state
Sessions in failed state | Sessions on the VR that are in the failed state
Dial-out target statistics | Statistics at the route target level
Targets active | Current active targets
Targets created | All targets created
Targets removed | Targets deleted
Targets in down state | Targets in the down state
Targets in inhibited state | Targets in the inhibited state
Targets in in-service state | Targets in the inService state
Triggers discarded | Trigger packets discarded
Dial-out session statistics | Statistics at the session level
Sessions active | Currently active sessions
Sessions created | All sessions created
Sessions removed | Sessions deleted
Sessions reset | Sessions reset using the l2tp dial-out session reset command
Triggers received | Triggers received for dial-out sessions
Triggers enqueued | Triggers that have been put into the queue
Triggers discarded | Trigger packets discarded
Triggers forwarded | Trigger packets forwarded
Triggers max enqueued | Maximum number of triggers that have been enqueued simultaneously since the last router reset
Authentication requests | Authentication requests received
No resources for authentication | Authentication requests not processed because of insufficient resources
Authentication grants | Authentication requests granted
Authentication Denies | Authentication requests denied
Dial-outs requested | Outgoing calls requested for sessions
Dial-outs rejected | Outgoing call requests that were rejected
Dial-outs established | Successful outgoing calls before the connecting timer expired
Dial-outs timed out | Number of times the connecting timer expired
Dial-outs torn down | Successful outgoing calls that were terminated

#### Related Topics

- For detailed information about operational states, see Dial-Out Operational States
- show l2tp dial-out
- show l2tp dial-out virtual-router