Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Related Topics
- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass traffic-class

# Configuring Traffic Classes on Multiclass MLPPP Interfaces

You can configure mapping of QoS traffic classes to multilink classes. The best-effort QoS traffic class is mapped to multilink class 0 by default.

To configure mapping of QoS traffic classes to multilink classes:

- Specify the QoS traffic classes to be mapped to the multilink classes.

  - To map QoS traffic classes to multilink classes in a dynamic profile:

    host1(config-profile)#ppp multilink multiclass traffic-class best-effort voice otherData video

  - To map QoS traffic classes to multilink classes in a static MLPPP interface:

    host1(config-if)#ppp multilink multiclass traffic-class best-effort voice otherData video

  | Note: You must include the best-effort traffic class in the ppp multilink multiclass traffic-class command, or the command fails.

#### Related Topics

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass traffic-class

#### Published: 2010-07-07

Help
|
My Account
|
Log Out